- Top
- CCU menu
- MAINTENANCE
- NETWORK(1/2)

# NETWORK(1/2)

This is the selection screen for the NETWORK(1/2) menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
IP ADDRESS | (Factory setting: 192.168.0.20) | Set the IP address. Select and set each set of three digits with the cursor.
SUBNETMASK | (Factory setting: 255.255.255.0) | Set the subnet mask.
DEFAULT GATEWAY | (Factory setting: 192.168.0.1) | Set the default gateway.
HTTP PORT | 00001 to 00080 to 65535 | Set the port number used for web access.
ROP PORT | 49152 to 49200 to 49299 | Set the port number used for connecting to the ROP.
SET EXECUTE | - | When you press the [SELECT] button, [NETWORK SET EXECUTE NO/YES] appears. Select [YES] to apply the configured [NETWORK] information to the unit. If this operation is not performed, the changed [NETWORK] settings will not be applied. In addition, if you exit the menu without performing this operation, the settings will return to their original values.
MAC ADDRESS | Display only | Displays the MAC address.

Top of the page