- Top
- Connection
- System configuration
- IP connection

# IP connection

Use the optical fiber multi cable (sold separately) to connect the unit and camera.

Connect the unit to the ROP (AK-HRP1000 / AK-HRP1005 / AK-HRP1010 / AK-HRP1015 / AK-HRP250) via a PoE-compatible switching hub using LAN cables (straight cables: sold separately).

- Read “Network security” before connecting the devices.

- Use a switching hub with PoE support.

For the connection procedure, see "Equipment connections."

“Equipment connections”

Top of the page