- Top
- CCU menu
- OPERATION
- HD PHASE

# HD PHASE

This is the selection screen for the HD PHASE menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
HD H COARSE | -127 to 0 to +127 | Make the coarse setting of the H_FINE phase used with GL HD REF.
HD H FINE | -100 to 0 to +100 | Make the fine setting of the H_FINE phase used with GL HD REF.
V ADVANCE | -3 / -2 / -1 / 0 | Set the vertical phase of this unit in relation to the vertical phase of the REF signal. The larger the negative value, the larger the advance. The setting unit varies depending on [CCU MODE]. When the mode is [720/59p] or [720/50p], the setting unit is 1H of [720p]. When the mode is [1080/23.98psF], the setting unit is 1H of [1080/23.98psF]. Otherwise, the setting unit is 1H of [1080/59i] or [1080/50i].

Top of the page