- Top
- Web Screen (AK-NP600)
- Displaying the web screen (AK-NP600)
- Network settings screen [Network]

# Network settings screen [Network]

Make settings related to the network for AK-NP600 in the Network settings screen [Network].

The Network settings screen [Network] consists of [SFP+ primary], [SFP+ primary TX], [SFP+ primary RX], [SFP+ secondary], [SFP+ secondary TX], [SFP+ secondary RX], [1GbE], [Tally in setting], [PTP setting], [NMOS setting], and [Common].

#### SFP+ primary

Click [SFP+ primary] in the Network settings screen [Network].

Make network settings for the [SFP+1] slot (SFP+ primary) for MoIP input/output.

Confirm the settings with the [Set] button.

The following information is required to configure network settings. Consult your network administrator or Internet service provider.

IP address

Port

Subnet mask

Default gateway (when using a gateway server or router)

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
DHCP | ON OFF | Select the method for setting the SFP+ primary IP addresses.
IP address | 192.168.0.50 | When not using the DHCP function, enter the SFP+ primary IP addresses. Enter so that the address does not duplicate the IP addresses of the personal computer or other network cameras.
Port | 49300 (1024 to 50000) | Enter the SFP+ primary port numbers.
Subnet mask | 255.255.255.0 | When not using the DHCP function, enter the SFP+ primary subnet masks.
Default gateway | 192.168.0.1 | When not using the DHCP function, set the SFP+ primary default gateways.
Mac address | Display only | Display the SFP+ primary MAC addresses.

#### SFP+ primary TX

Click [SFP+ primary TX] in the Network settings screen [Network].

Make network settings for the SFP+ primary TX signal.

Confirm the settings with the [Set] button.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
Main video TX | IP address 224.1.0.1 Port 49301 (1024 to 50000, 10670 is prohibited) | IP address Enter the IP address for Main video TX. Port Enter the port number for Main video TX.
Monitor video TX | IP address 224.1.0.2 Port 49302 (1024 to 50000, 10670 is prohibited) | IP address Enter the IP address for Monitor video TX. Port Enter the port number for Monitor video TX.
HD trunk TX | IP address 224.1.0.10 Port 49310 (1024 to 50000, 10670 is prohibited) | IP address Enter the IP address for HD trunk TX. Port Enter the port number for HD trunk TX.
MIC1 audio TX | IP address 224.1.0.3 Port 49303 (1024 to 50000, 10670 is prohibited) | IP address Enter the IP address for MIC1 audio TX. Port Enter the port number for MIC1 audio TX.
MIC2 audio TX | IP address 224.1.0.11 Port 49311 (1024 to 50000, 10670 is prohibited) | IP address Enter the IP address for MIC2 audio TX. Port Enter the port number for MIC2 audio TX.
INCOM1 audio TX | IP address 224.1.0.12 Port 49312 (1024 to 50000, 10670 is prohibited) | IP address Enter the IP address for INCOM1 audio TX. Port Enter the port number for INCOM1 audio TX.
INCOM2 audio TX | IP address 224.1.0.13 Port 49313 (1024 to 50000, 10670 is prohibited) | IP address Enter the IP address for INCOM2 audio TX. Port Enter the port number for INCOM2 audio TX.

#### SFP+ primary RX

Click [SFP+ primary RX] in the Network settings screen [Network].

Make network settings for the SFP+ primary RX signal.

Confirm the settings with the [Set] button.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
Return video RX | Multicast address 224.1.0.4 Source address 0.0.0.0 Port 49304 (1024 to 50000, 10670 is prohibited) | Multicast address Enter the multicast address for return images. Source address Enter the source IP address for return images. Port Enter the port number for return images.
HD prompter RX | Multicast address 224.1.0.14 Source address 0.0.0.0 Port 49314 (1024 to 50000, 10670 is prohibited) | Multicast address Enter the multicast address for HD PROMPTER RX. Source address Enter the source IP address for HD PROMPTER RX. Port Enter the port number for HD PROMPTER RX.
PGM1 audio RX | Multicast address 224.1.0.16 Source address 0.0.0.0 Port 49316 (1024 to 50000, 10670 is prohibited) | Multicast address Enter the multicast address for PGM1 audio RX. Source address Enter the source IP address for PGM1 audio RX. Port Enter the port number for PGM1 audio RX.
PGM2 audio RX | Multicast address 224.1.0.17 Source address 0.0.0.0 Port 49317 (1024 to 50000, 10670 is prohibited) | Multicast address Enter the multicast address for PGM2 audio RX. Source address Enter the source IP address for PGM2 audio RX. Port Enter the port number for PGM2 audio RX.
INCOM1 audio RX | Multicast address 224.1.0.18 Source address 0.0.0.0 Port 49318 (1024 to 50000, 10670 is prohibited) | Multicast address Enter the multicast address for INCOM1 audio RX. Source address Enter the source IP address for INCOM1 audio RX. Port Enter the port number for INCOM1 audio RX.
INCOM2 audio RX | Multicast address 224.1.0.19 Source address 0.0.0.0 Port 49319 (1024 to 50000, 10670 is prohibited) | Multicast address Enter the multicast address for INCOM2 audio RX. Source address Enter the source IP address for INCOM2 audio RX. Port Enter the port number for INCOM2 audio RX.

#### SFP+ secondary

Click [SFP+ secondary] in the Network settings screen [Network].

Make network settings for the [SFP+2] slot (SFP+ secondary) for MoIP input/output.

Confirm the settings with the [Set] button.

The following information is required to configure network settings. Consult your network administrator or Internet service provider.

IP address

Port

Subnet mask

Default gateway (when using a gateway server or router)

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
DHCP | ON OFF | Select the method for setting the SFP+ secondary IP addresses.
IP address | 192.168.0.51 | When not using the DHCP function, enter the SFP+ secondary IP addresses. Enter so that the address does not duplicate the IP addresses of the personal computer or other network cameras.
Port | 49309 (49300 to 49999) | Enter the SFP+ secondary port numbers.
Subnet mask | 255.255.255.0 | When not using the DHCP function, enter the SFP+ secondary subnet masks.
Default gateway | 192.168.0.1 | When not using the DHCP function, set the SFP+ secondary default gateways.
Mac address | Display only | Display the SFP+ secondary MAC addresses.

#### SFP+ secondary TX

Click [SFP+ secondary TX] in the Network settings screen [Network].

Make network settings for the SFP+ secondary TX signal.

Confirm the settings with the [Set] button.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
Main video TX | IP address 224.1.0.5 Port 49305 (1024 to 50000, 10670 is prohibited) | IP address Enter the IP address for Main video TX. Port Enter the port number for Main video TX.
Monitor video TX | IP address 224.1.0.6 Port 49306 (1024 to 50000, 10670 is prohibited) | IP address Enter the IP address for Monitor video TX. Port Enter the port number for Monitor video TX.
HD trunk TX | IP address 224.1.0.20 Port 49320 (1024 to 50000, 10670 is prohibited) | IP address Enter the IP address for HD trunk TX. Port Enter the port number for HD trunk TX.
MIC1 audio TX | IP address 224.1.0.7 Port 49307 (1024 to 50000, 10670 is prohibited) | IP address Enter the IP address for MIC1 audio TX. Port Enter the port number for MIC1 audio TX.
MIC2 audio TX | IP address 224.1.0.21 Port 49321 (1024 to 50000, 10670 is prohibited) | IP address Enter the IP address for MIC2 audio TX. Port Enter the port number for MIC2 audio TX.
INCOM1 audio TX | IP address 224.1.0.22 Port 49322 (1024 to 50000, 10670 is prohibited) | IP address Enter the source IP address for INCOM1 audio TX. Port Enter the port number for INCOM1 audio TX.
INCOM2 audio TX | IP address 224.1.0.23 Port 49323 (1024 to 50000, 10670 is prohibited) | IP address Enter the source IP address for INCOM2 audio TX. Port Enter the port number for INCOM2 audio TX.

#### SFP+ secondary RX

Click [SFP+ secondary RX] in the Network settings screen [Network].

Make network settings for the SFP+ secondary RX signal.

Confirm the settings with the [Set] button.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
Return video RX | Multicast address 224.1.0.8 Source address 0.0.0.0 Port 49308 (1024 to 50000, 10670 is prohibited) | Multicast address Enter the multicast address for return images. Source address Enter the source IP address for return images. Port Enter the port number for return images.
HD prompter RX | Multicast address 224.1.0.24 Source address 0.0.0.0 Port 49324 (1024 to 50000, 10670 is prohibited) | Multicast address Enter the multicast address for HD PROMPTER RX. Source address Enter the source IP address for HD PROMPTER RX. Port Enter the port number for HD PROMPTER RX.
PGM1 audio RX | Multicast address 224.1.0.26 Source address 0.0.0.0 Port 49326 (1024 to 50000, 10670 is prohibited) | Multicast address Enter the multicast address for PGM1 audio RX. Source address Enter the source IP address for PGM1 audio RX. Port Enter the port number for PGM1 audio RX.
PGM2 audio RX | Multicast address 224.1.0.27 Source address 0.0.0.0 Port 49327 (1024 to 50000, 10670 is prohibited) | Multicast address Enter the multicast address for PGM2 audio RX. Source address Enter the source IP address for PGM2 audio RX. Port Enter the port number for PGM2 audio RX.
INCOM1 audio RX | Multicast address 224.1.0.28 Source address 0.0.0.0 Port 49328 (1024 to 50000, 10670 is prohibited) | Multicast address Enter the multicast address for INCOM1 audio RX. Source address Enter the source IP address for INCOM1 audio RX. Port Enter the port number for INCOM1 audio RX.
INCOM2 audio RX | Multicast address 224.1.0.29 Source address 0.0.0.0 Port 49329 (1024 to 50000, 10670 is prohibited) | Multicast address Enter the multicast address for INCOM2 audio RX. Source address Enter the source IP address for INCOM2 audio RX. Port Enter the port number for INCOM2 audio RX.

#### 1GbE

Click [1GbE] in the Network settings screen [Network].

Make network settings for the 1GbE (LAN2) for AK-NP600.

Confirm the settings with the [Set] button.

The following information is required to configure network settings. Consult your network administrator or Internet service provider.

IP address

Port

Subnet mask

Default gateway (when using a gateway server or router)

Primary server address, secondary server address, and domain for DNS (when using DNS)

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
DHCP | ON OFF | Select the method for setting the 1GbE (LAN2) IP addresses.
IP address | 192.168.0.52 | When not using the DHCP function, enter the 1GbE (LAN2) IP addresses. Enter so that the address does not duplicate the IP addresses of the personal computer or other network cameras.
Port | 49330 (1024 to 50000) | Enter the 1GbE (LAN2) port numbers.
Subnet mask | 255.255.255.0 | When not using the DHCP function, enter the 1GbE (LAN2) subnet masks.
Default gateway | 192.168.0.1 | When not using the DHCP function, set the 1GbE (LAN2) default gateways.
Mac address | Display only | Display the 1GbE (LAN2) MAC addresses.
DNS | DNS MANUAL AUTO Primary server address 0.0.0.0 Secondary server address 0.0.0.0 Domain The default value is blank | DNS Sets whether the DNS server address is to be acquired automatically (AUTO), or to be input manually (MANUAL). Primary server address Secondary server address Domain When using [MANUAL] for [DNS], enter the IP address for the DNS server. Consult the system administrator regarding the DNS server information.

#### Tally in setting

Click [Tally in setting] in the Network settings screen [Network].

Make settings related to Tally control via TSL Protocol 5.0.

Confirm the settings with the [Set] button.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
Index no. | 1 (1 to 65534) | Enter the Index no. set by devices that output Tally.
Port | 62000 (60000 to 65535) | Enter the Tally in port number.

NOTE

- The IP address of Tally in becomes the setting of the connected IP network.
  Ex.: When input from SFP+ primary
  The SFP+ Primary IP address is enabled

#### PTP setting

Click [PTP setting] in the Network settings screen [Network].

Make PTP related network settings.

Confirm the settings with the [Set] button.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
Domain | 127 (0 to 127) | Sets the DOMAIN number.
IP address | Display only | Displays the IP address automatically discovered.

#### NMOS setting

Click [NMOS setting] in the Network settings screen [Network].

Make NMOS related network settings.

Confirm the settings with the [Set] button.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
NMOS control | ON OFF | Enables/disables the NMOS function.
Status | UNREGISTERD REGISTERING REGISTERED P2P MODE (Display only) | Displays the NMOS operation status, such as RDS connection status.
Port(IS-04) | 50040 (1024 to 65535) | Sets the port number on the camera for IS-04 Node API.
Port(IS-05) | 50050 (1024 to 65535) | Sets the port number on the camera for IS-05 Node API.
RDS IP address | Display only | Displays the discovered IP address.
RDS port | Display only | Displays the port number automatically discovered.
Label setting | AUTO MANUAL | AUTO The Label prefix cannot be changed. It is fixed to UCU600_**** ("****" is the last four digits of the Mac address). MANUAL Text can be set in Label prefix.
Index no. | UCU600_**** (“****” is the last four digits of the Mac address) | Sets the prefix appended which is shared with NMOS resource names on this unit.
Port | uniDNS mDNS | Sets the method for NMOS resource discovery.

#### Common

Click [Common] in the Network settings screen [Network].

Make AK-NP600 shared network settings.

Confirm the settings with the [Set] button.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
EasyIP Setup accommodate period | 20min. Unlimited | Sets the time allowed for network setting operations from EasyIP Setup Tool Plus. 20min. Allows camera setting operations on the EasyIP Setup Tool Plus for just 20 minutes after start up of this unit. Unlimited Allows camera setting operations on the EasyIP Setup Tool Plus at any time. Camera display on the EasyIP Setup Tool Plus is enabled all the time, and the camera screen can be opened. Consult the network administrator regarding the address settings for the different servers.
EasyIP Setup Plus plain text usage | Enable Disable | Sets whether to enable or disable encryption of communications when communicating with EasyIP Setup Tool Plus. Enable. Communications are sent and received as plain messages. Disable Communications are sent and received as encrypted messages.

Top of the page