- Top
- Parts and their functions
- Front panel 2

# Front panel 2

1 | [STATUS] indicators | Lights to indicate the unit status. [G/L ON] indicator Lights when the external sync signal is synchronized. “Front panel [G/L ON] indicator specifications” [FAN] indicator Lights when the rotation speed of the unit's cooling fan drops below the normal value. [ALARM] indicator Lights when the unit malfunctions.
2 | [CABLE] indicators | Lights to indicate the cable connection status. [NORMAL] indicator This lights when the unit and camera are properly connected by the optical fiber multi cable. [OPEN] indicator This lights when the unit and camera are not connected by the optical fiber multi cable. [SHORT] indicator This lights when the cable connecting the unit and camera has been short-circuited.
3 | [PRIV/SYSTEM] selector switch | This switch is for selecting the party to call using the intercom. Switch position
PRIV: | For making private calls between the unit and camera side.
SYSTEM: | For calling the intercom on the system side and camera side.
4 | [PRIV] indicator | Lights when the [PRIV/SYSTEM] selector switch is set to PRIV.
5 | [PROD/BOTH/ENG] selector switch | This switch selects the party to which to speak via the intercom.
6 | [MIC] switch | This switch switches the intercom microphone ON/OFF. Switch position
ON: | The intercom microphone is turned on.
OFF: | The intercom microphone is turned off.
PTT: | The intercom microphone is on only while the switch is held down.
7 | [PGM] switch | This switch mixes audio for the intercom. Switch position
PGM1: | The sound of PGM1 is mixed with the intercom sound.
OFF: | The sound of PGM is not mixed with the intercom sound.
PGM2: | The sound of PGM2 is mixed with the intercom sound.
8 | [INCOM LEVEL] adjustment dial | These controls are for adjusting the volume level of the sound heard through the intercom.
9 | [PGM LEVEL] adjustment dial | This dial adjusts the volume level of the intercom's program audio mix.
10 | [CALL] button | This button calls the camera and the ROP. During calling, it lights red.

Top of the page