- Top
- CCU menu
- OPERATION
- OUT FORMAT(UHD_HDR)

# OUT FORMAT(UHD_HDR)

This is the selection screen for the OUT FORMAT(UHD_HDR) menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
SDI OUT1-4 SDI OUT1 | UHD_HDR UHD_HDR (12G) UHD_HDR (6G) | Displays the format of the signals to be output from [1] to [4] of the [UHD/HS/HD SDI OUT] connectors. The content selected in SDI OUT1-4 is displayed for the items of SDI OUT1-4. When there is no output, "no signal" will be displayed. “Output selection conditions”
SDI OUT1-4 SDI OUT2
SDI OUT1-4 SDI OUT3
SDI OUT1-4 SDI OUT4
SDI OUT5&6 | 3G_HDR HD_HDR 3G_SDR HD_SDR PsF_HDR TrueP_HDR OVER(3G) PsF_SDR TrueP_SDR OVER(3G)_SDR | Set the format of the signals to be output from [5] to [7] of the [HD SDI OUT] connectors. When [CCU MODE] is set to [2160/29.97p], [2160/23.98p], [2160/25p], [2160/29.97PsF], [2160/23.98PsF] or [2160/25PsF]: PsF_HDR/PsF_SDR/TrueP_HDR/TrueP_SDR/OVER(3G)_HDR/OVER(3G)_SDR With PsF/TrueP/OVER(3G), the settings made for SDI OUT5&6 are reflected in SDI OUT7, and only switching between HDR/SDR is possible in SDI OUT7. When [CCU MODE] is other than [2160/29.97p], [2160/23.98p], [2160/25p], [2160/29.97PsF], [2160/23.98PsF], [2160/25PsF]: 3G_HDR/3G_SDR/HD_HDR/HD_SDR “Output selection conditions”
SDI OUT7
SDI OUT8 | HD_HDR HD_SDR PsF_HDR PsF_SDR | Set the format of the signals to be output from [8/PM] of the [HD SDI OUT] connector. When [CCU MODE] is set to [2160/29.97p], [2160/23.98p], [2160/25p], [2160/29.97PsF], [2160/23.98PsF] or [2160/25PsF]: PsF_HDR/PsF_SDR When [CCU MODE] is other than [2160/29.97p], [2160/23.98p], [2160/25p], [2160/29.97PsF], [2160/23.98PsF], [2160/25PsF]: HD_HDR/HD_SDR “Output selection conditions”
SDI OUT8 NORMAL/PM | PM NORMAL | Set the signal to be output from [8/PM] of the [HD SDI OUT] connector. Can only be set to PM when using a MoIP board (AK-NP600). PM : Output the picture monitor images. NORMAL : Output the main line images.
OUTPUT FORMAT | INTERLEAVE SQUARE | Set the format (INTERLEAVE/SQUARE) of the UHD signals to be output from [1] to [4] of the [UHD/HS/HD SDI OUT] connectors. When [CCU MODE] is set to [2160/29.97psF], [2160/23.98psF], [2160/25psF] or [2160/23psF & over59i]: SQUARE (fixed)
3G SDI | LEVEL-A LEVEL-B | Set the output format for 3G output.
HD SDI FORMAT | 1080i 1080p 720p | Set the format for when the output format for SDI 5 to 8 is HD_HDR. When [CCU MODE] is [2160/59.94p]: 1080i/720p When [CCU MODE] is [2160/29.97p], [2160/23.98p], [2160/29.97psF], [2160/23.98psF] or [2160/23PsF & over59i]: 1080p (fixed) When [CCU MODE] is [2160/50p]: 1080i When [CCU MODE] is [2160/25p] or [2160/25psF]: 1080p (fixed)
HD TRUNK/TICO | HD_TRUNK TICO | Set the signal to be output from the [HD TRUNK/TICO OUT] connector. HD_TRUNK: Outputs the signals compatible with HD_TRUNK. TICO: Outputs the signals compatible with TICO.
HDR COLORIMETRY | BT.709 BT.2020 | Change the Y/C conversion coefficient.
GAMUT | NORMAL WIDE_G WIDE_G2 | Change the color gamut. Applies only to the signals output from the [SDI OUT 1] to [SDI OUT 4] connectors. This will be NORMAL/WIDE_G when AK-UC3000 is connected. This will be NORMAL/WIDE_G2 when AK-PLV100 is connected.

#### With AK-NP600 option

FORMAT/ CCU MODE | SDI | ANALOG
--- | --- | ---
OUT1 | OUT2 | OUT3 | OUT4 | OUT5 | OUT6 | OUT7 | OUT8 | COMPOSITE /PM
UHD_HDR (59.94)
| 2160 /59.94p | UHD_HDR (12G) | no signal | 3G_HDR, 3G_SDR, HD_HDR, HD_SDR | HD_HDR, HD_SDR | NORMAL /PM
UHD_HDR
2160 /29.97p | UHD_HDR (6G) | no signal | PsF_HDR, PsF_SDR, TrueP_HDR, TrueP_SDR, OVER(3G)_HDR, OVER(3G)_SDR | PsF_HDR, PsF_SDR | NORMAL /PM
UHD_HDR
2160 /23.98p | UHD_HDR (6G) | no signal | PsF_HDR, PsF_SDR, TrueP_HDR, TrueP_SDR, OVER(3G)_HDR, OVER(3G)_SDR | PsF_HDR, PsF_SDR | NORMAL /PM
UHD_HDR
2160 /29.97PsF | UHD_HDR | PsF_HDR, PsF_SDR, TrueP_HDR, TrueP_SDR, OVER(3G)_HDR, OVER(3G)_SDR | PsF_HDR, PsF_SDR | NORMAL /PM
2160 /23.98PsF | UHD_HDR | PsF_HDR, PsF_SDR, TrueP_HDR, TrueP_SDR, OVER(3G)_HDR, OVER(3G)_SDR | PsF_HDR, PsF_SDR | NORMAL /PM
2160 /23.98PsF & over 59i | UHD_HDR | HD_HDR, HD_SDR | NORMAL /PM
UHD_HDR (50)
| 2160 /50p | UHD_HDR (12G) | no signal | 3G_HDR, 3G_SDR, HD_HDR, HD_SDR | HD_HDR, HD_SDR | NORMAL /PM
UHD_HDR
2160 /25p | UHD_HDR (6G) | no signal | PsF_HDR, PsF_SDR, TrueP_HDR, TrueP_SDR, OVER(3G)_HDR, OVER(3G)_SDR | PsF_HDR, PsF_SDR | NORMAL /PM
UHD_HDR
2160 /25PsF | UHD_HDR | PsF_HDR, PsF_SDR, TrueP_HDR, TrueP_SDR, OVER(3G)_HDR, OVER(3G)_SDR | PsF_HDR, PsF_SDR | NORMAL /PM

Top of the page