- Top
- Notes
- Recording function that cannot be used simultaneously

# Recording function that cannot be used simultaneously

Depending on the recording function that is set, there are recording functions that cannot be used simultaneously.

- Meaning of the symbols used in the table are as follows.

  - ✓: Can be used simultaneously.

  - —: Cannot be used simultaneously.

| Recording function that is set
--- | ---
Recording function to additionally set | Pre-recording*1*2*3 | Relay recording*3 | Simultaneous recording*3 | Interval recording*3*4*5*6*7*8 | VFR*4*5*6
Pre-recording*1*2*3 |  | ✓ | ✓ | — | —
Relay recording*3 | ✓ |  | — | — | ✓*9
Simultaneous recording*3 | ✓ | — |  | ✓ | ✓*9
Interval recording*3*4*5*6*7*8 | — | — | ✓ |  | —
VFR*4*5*6 | — | ✓*9 | ✓*9 | — |

Time code is fixed to free run.

The pre-recording is cancelled once when three hours has passed without starting the recording.

When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF], this cannot be set.

Cannot set simultaneously in the following cases.

- When recording in AVCHD format

Time code is fixed to recording run.

When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [FREQUENCY] is set to [50.00i]/[59.94i], this cannot be set.

The time code is fixed to [NDF].

The [OUTPUT SETTINGS] menu → [SDI OUT] → [SDI REC REMOTE] and the [OUTPUT SETTINGS] menu → [HDMI OUT] → [HDMI REC REMOTE] will not operate.

The function will not operate if the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SENSOR MODE] is set to [S35 MIX 2.8K] or [4/3 CROP&MIX 2.2K].

Top of the page