- Top
- Preparation
- Setting of time data
- Supplying the time code externally

# Supplying the time code externally

The time code output from the camera corresponding to the camera video or the playback video can be supplied to an external recording device.

<SDI OUT> terminal

SDI IN terminal

VTR, etc.

TC IN terminal

<TC IN/OUT> terminal

Select the [REC SETTINGS] menu → [TC] → [TC IN/OUT SEL] → [TC OUT].

Select the [REC SETTINGS] menu → [TC] → [TC OUT REF] → [RECORDING].

The same time code can be recorded to the video of the same time on two devices.

#### To match the time code output from the <TC IN/OUT> terminal to the video of the SDI output or the monitor output

Select the [REC SETTINGS] menu → [TC] → [TC OUT REF] → [SDI OUT].

NOTE

- TCR is output during playback. TCG output during playback is not supported.

- When [FREQUENCY] is [23.98p] or [24.00p], time code output may be off by 1 frame.

- External locks by user bits are not supported.

Top of the page