- Top
- Shooting
- Convenient shooting functions
- Level gauge

# Level gauge

A level gauge that indicates the horizontal and vertical inclinations of the camera can be displayed on the LCD monitor.

The line of the level gauge is displayed in orange while the camera is inclined. The line of the level gauge will change from orange to light blue, and then to white when the inclination of the camera is corrected. It will indicate up to approximately 30° in horizontal direction, and 30° in vertical direction.

Select the [OUTPUT SETTINGS] menu → [LCD LEVEL GAUGE] → [LEVEL GAUGE] → [ON].

NOTE

- The display of level gauge cannot be recorded.

- The level gauge is not displayed when the enlarged display function of the focus assist function is enabled, or when displaying the color bars.

- The level gauge may not display correctly while moving the camera.

- The level gauge may not display correctly when shooting with the camera inclined excessively upward or downward.

- Displays/hides of the level gauge can be switched by pressing the USER button assigned with [LEVEL GAUGE].

- Current horizontal and vertical direction can be set as the reference value of the level gauge by pressing the USER button assigned with [LEVEL GAUGE RESET]. To restore the set value, set with the [OUTPUT SETTINGS] menu → [LCD LEVEL GAUGE] → [LEVEL GAUGE RESET].

Top of the page