- Top
- Shooting
- Image quality adjustment
- [WHITE]

# [WHITE]

## [ATW] (auto tracking white balance)

The camera is equipped with the auto tracking white balance (ATW) function that automatically tracks the white balance of images according to the lighting condition.

This function does not guarantee 100% accuracy for the white balance. There is some range in the the tracking against the change in the lighting condition or accuracy in the white balance. Take care when using this function.

## [AWB] (auto white balance)

Place a white pattern in a point where the light condition matches the light source for the subject, and display white in the screen.

Adjust the luminance with the <IRIS> dial.

Select the [CAMERA SETTINGS] menu → [WHITE] → [VALUE] → [AWB MEMORY A]/[AWB MEMORY B].

Select the [CAMERA SETTINGS] menu → [WHITE] → [AWB] → [EXECUTE].

- It will operate the same by pressing the USER button assigned with [AWB] (auto white balance).

#### Adjustment value

- The adjusted value is saved automatically in [AWB MEMORY A]/[AWB MEMORY B].

#### White pattern

- A white object (cloth or wall) near the subject may also be used for the white pattern.

- Required size of white pattern is as follows.

  1/2 or more of the screen width

  1/2 or more of the screen height

- Keep bright spotlights out of the screen.

- The white pattern must be placed at the center of the screen.

## Manually setting the color temperature (setting with [VALUE])

Can be selected from the up to 13 registered color temperatures (white balance).

Select the [CAMERA SETTINGS] menu → [WHITE] → [VALUE].

Select the color temperature.

Top of the page