- Top
- Operation
- Menu setting contents
- [SCENE FILE SETTINGS] menu

# [SCENE FILE SETTINGS] menu

Sets the detailed image quality adjustment of the camera video.

This menu cannot be set when the thumbnail screen is displayed.

For factory settings, refer to “Factory setting value of the scene file”.

## [NAME EDIT]

Edits the name of the scene file selected in the [SYSTEM SETTINGS] menu → [COLOR SETTINGS] → [MAIN]. (Maximum eight characters)

## [SCENE DATA]

For saving and loading target, refer to “Target items for scene file/setup file/initialization”.

For details of saving and loading, refer to “Handling setting data”.

### [LOAD]

Loads the scene file saved in the camera memory, and reflects to the current setting value.

The items that can be selected are as follows.

- [YES], [NO]

### [SAVE]

Saves the current setting value as a scene file into the camera memory.

The items that can be selected are as follows.

- [YES], [NO]

### [INITIALIZE]

Returns the current setting value of the scene file to the factory setting.

The items that can be selected are as follows.

- [YES], [NO]

## [BLACK]

Adjusts the standard black level.

### [M.PED]

Adjusts the standard black level for the entire video.

The items that can be set are as follows.

- [−100]…[100]

### [R PED]

Adjust the standard black level for Rch.

The items that can be set are as follows.

- [−100]…[100]

### [G PED]

Adjust the standard black level for Gch.

The items that can be set are as follows.

- [−100]…[100]

### [B PED]

Adjust the standard black level for Bch.

The items that can be set are as follows.

- [−100]…[100]

### [PEDESTAL OFFSET]

Sets the standard black level for Rch, Gch, and Bch when the auto black balance adjustment is executed.

[ON] | The values for [R PED], [G PED], and [B PED] are maintained even after the auto black balance adjustment is executed.
[OFF] | Resets the values of the [R PED], [G PED], and [B PED] after executing the auto black balance adjustment.

## [GAMMA]

### [GAMMA SELECT]

Selects the gamma mode.

[V-255570L1] | A gamma curve for EVA-LOOK.
[V-504580L1] | A gamma curve for EVA-LOOK.
[VIDEO] | A gamma curve for BroadCast-LOOK.
[HLG] | A hybrid log gamma (HLG) curve.

### [MASTER GAMMA]

Sets the master gamma in 0.01 steps.

The items that can be set are as follows.

- [0.30]…[0.75]

### [BLACK GAMMA]

Sets the gamma curves of dark areas.

The items that can be set are as follows.

[−8]…[−1] | Compresses the dark area.
[OFF] | Standard condition.
[1]…[8] | Expands the dark area.

### [B.GAMMA RANGE]

Sets the maximum level to perform compression/expansion of dark area.

The items that can be set are as follows.

[1] | Around 20%
[2] | Around 30%
[3] | Around 40%

## [KNEE]

### [KNEE SW]

Enables/disables operation of the knee.

The items that can be set are as follows.

- [ON], [OFF]

### [KNEE MODE]

Sets the knee operation mode.

[D RANGE] | The dynamic range that can be represented is determined by the value of [KNEE SLOPE] in [KNEE]. The value of dynamic range that can be represented does not change even when the value of [KNEE POINT] in [KNEE] is changed.
[PRESS] | The compression rate of the signal is determined by the value of [KNEE SLOPE] in [KNEE]. The value of dynamic range that can be represented will change when the value of [KNEE POINT] in [KNEE] is changed.

### [KNEE POINT]

Sets the position of the knee point.

The items that can be set are as follows.

- [75%]…[109%] (1% steps)

### [KNEE SLOPE]

Sets the knee inclination.

The items that can be set are as follows.

- [0]…[100]

## [HLG KNEE]

### [KNEE SW]

Enables/disables the operation of knee for HLG.

The items that can be set are as follows.

- [ON], [OFF]

### [KNEE POINT]

Sets the position of the knee point for HLG.

The items that can be set are as follows.

- [55]…[100] (1 steps)

### [KNEE SLOPE]

Sets the inclination of knee for HLG.

The items that can be set are as follows.

- [0]…[100]

## [WHITE CLIP]

### [SW]

Switches the enable/disable of the white clip function.

The items that can be set are as follows.

- [ON], [OFF]

### [LEVEL]

Sets the level of the white clip.

The items that can be set are as follows.

- [90%]…[109%]

## [DETAIL]

### [SW]

Switches the enable/disable of the detail function.

The items that can be set are as follows.

- [ON], [OFF]

### [CORING]

Sets the level of coring against the detail.

The items that can be set are as follows.

- [0]…[60]

### [MASTER LEVEL]

Sets the level of the detail effect of the whole part.

The items that can be set are as follows.

- [−31]…[31]

### [FREQUENCY]

Sets the thickness of the detail.

The items that can be set are as follows.

- [1]…[3]

## [SKIN DETAIL]

### [SKIN DTL1]

Selects the skin tone table of the subject to apply the skin tone, and enables/disables the skin tone detail function.

The items that can be set are as follows.

- [ON], [OFF]

### [SKIN DTL2]

Selects the skin tone table of the subject to apply the skin tone, and enables/disables the skin tone detail function.

The items that can be set are as follows.

- [ON], [OFF]

### [SKIN DTL3]

Selects the skin tone table of the subject to apply the skin tone, and enables/disables the skin tone detail function.

The items that can be set are as follows.

- [ON], [OFF]

## [CHROMA]

### [LEVEL]

Sets the chroma level of PR and PB signals.

The items that can be set are as follows.

- [OFF], [−99%]…[99%]

## [MATRIX]

### [SW]

Enables/disables the matrix function.

The items that can be set are as follows.

- [ON], [OFF]

### [(R-G)]

Adjusts the linear matrix. (Red - Green)

The items that can be set are as follows.

- [−127]…[127]

### [(R-B)]

Adjusts the linear matrix. (Red - Blue)

The items that can be set are as follows.

- [−127]…[127]

### [(G-R)]

Adjusts the linear matrix. (Green - Red)

The items that can be set are as follows.

- [−127]…[127]

### [(G-B)]

Adjusts the linear matrix. (Green - Blue)

The items that can be set are as follows.

- [−127]…[127]

### [(B-R)]

Adjusts the linear matrix. (Blue - Red)

The items that can be set are as follows.

- [−127]…[127]

### [(B-G)]

Adjusts the linear matrix. (Blue - Green)

The items that can be set are as follows.

- [−127]…[127]

## [COLOR CORRECTION]

For details of setting, refer to “[COLOR CORRECTION]”.

[SW] | Enables/disables the color correction function. The items that can be set are as follows. [ON], [OFF]
[PARAM] | This function sets color saturation and phase. It can be set to individual color hue. The items that can be set are as follows. [−63]…[63]

Top of the page