- Top
- Shooting
- Special recording function
- Interval recording

# Interval recording

The camera will record one frame at each set time interval.

1 frame recording

1 frame recording

1 frame recording

(Time)

Time set in [INTERVAL TIME]

Time set in [INTERVAL TIME]

Select the [REC SETTINGS] menu → [REC FUNCTION] → [REC MODE] → [INTERVAL].

[INTRVL] is displayed in the special recording function display of the VIEW screen and the HOME screen.

- When the recording mode is set to AVCHD, or when the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [FREQUENCY] is set to [50.00i]/[59.94i], this cannot be selected.

From the [REC SETTINGS] menu → [REC FUNCTION] → [INTERVAL TIME], set the time.

Press the REC button.

- [I-REC] is displayed in red in the special recording function display of the VIEW screen.

- The camera will repeat the operation of one frame recording at set time interval.

- To stop recording, press the REC button.

- To clear the setting, set the [REC SETTINGS] menu → [REC FUNCTION] → [REC MODE] to [NORMAL].

- The setting is not cleared even when the power is turned off.

NOTE

- Audio is not recorded.

- Recorded data (data recorded until recording was stopped) is included in one clip.

- The [REC SETTINGS] menu → [TC] → [FREE/REC RUN] is fixed to [REC RUN].

- The [REC SETTINGS] menu → [TC] → [DF/NDF] is fixed to [NDF].

- [SDI REC REMOTE] and [HDMI REC REMOTE] will not operate.

- If the length of the clip is less than three seconds when the recording is stopped, the image of the final frame will be recorded to make the length of the clip to three seconds.

- The recording is stopped once when the length of the clip exceeds ten hours in the interval recording. The recording is automatically resumed after few seconds.

- For recording limitation of the interval recording, refer to “Recording function that cannot be used simultaneously”.

Top of the page