- Top
- Shooting
- Convenient shooting functions
- Displaying frame marker

# Displaying frame marker

A frame marker can be displayed.

From the [OUTPUT SETTINGS] menu → [LCD MARKER] → [FRAME MARKER], select the angle of view.

- The frame marker is not displayed when [OFF] is selected.

## Setting the display color

From the [OUTPUT SETTINGS] menu → [LCD MARKER] → [FRAME COLOR], select the display color.

NOTE

- The marker cannot be recorded.

- When the enlarged display function and the focus square display of the focus assist function is enabled and while displaying the color bars, the marker is not displayed.

- Displays/hides of the marker can be temporarily switched by pressing the USER button with [LCD MARKER] assigned.

- The marker can be displayed in the output image from the <SDI OUT> terminal by setting in the [OUTPUT SETTINGS] menu → [SDI OUT] → [MARKER DISP] → [ON], and setting [SDI/HDMI MARKER]. Similarly, the marker can be displayed in the output image of the <HDMI> terminal by setting the [OUTPUT SETTINGS] menu → [HDMI OUT] → [MARKER DISP] → [ON].

Top of the page