- Top
- Specification
- Specifications
- Other input/output

# Other input/output

<TC IN/OUT> terminal | BNC×1 Used as input/output terminal, input/output switch by menu Input: 1.0 V - 4.0 V [p-p], 10 kΩ Output: 2.0 V±0.5 V [p-p], low impedance
<LCD> terminal | 40-pin (for connecting LCD monitor)
<REMOTE> terminal | 2.5 mm diameter super mini jack × 1, for connecting grip
<USB2.0 HOST> terminal | Type A connector, 4-pin (5 V, 0.5 A), for attaching the wireless module (optional)
<DC IN 12V> terminal | DC12 V, EIAJ type 4

Top of the page