- Top
- Output and Screen Display
- Screen status display

# Screen status display

#### During shooting

1. Clip name

   Displays the clip name being recorded with maximum of eight characters from beginning.

2. System resolution/RAW output resolution

   Displays the resolution set in the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [MAIN PIXEL]/[SENSOR MODE].

   - [4096×2160]

   - [3840×2160]

   - [2048×1080]

   - [1920×1080]

   - [1280×720]

   - [2048 MIX], [1920 MIX]: When [SENSOR MODE] is set to [S35 MIX 2.8K]

   - [2048 CROP], [1920 CROP]: When [SENSOR MODE] is set to [4/3 CROP&MIX 2.2K]

   When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF], the RAW output resolution set in [SDI RAW] is displayed.

   - [S35 5.7K]

   - [CROP 4K]

   - [CROP&MIX 2K]

3. System frequency

   Displays the frequency set in the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [FREQUENCY].

   - [23.98p]

   - [24.00p]

   - [25.00p]

   - [29.97p]

   - [50.00p]

   - [50.00i]

   - [59.94p]

   - [59.94i]

4. Color of the main recording

   Displays the color setting set in the [SYSTEM SETTINGS] menu → [COLOR SETTINGS] → [MAIN].

   - [VLog]: V-Log

   - [SCN1]: SCENE1

   - [SCN2]: SCENE2

   - [SCN3]: SCENE3

   - [SCN4]: SCENE4

   - [SCN5]: SCENE5

5. Recording format

   Displays the format set in the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [MAIN CODEC]/[SDI RAW].

   - [MOV HEVC]

   - [MOV 420L]

   - [MOV 422L]

   - [MOV 422I]

   - [AVCHD PS]

   - [AVCHD PH]

   - [AVCHD HA]

   - [AVCHD PM]

   - [SDI RAW]: When [SDI RAW] is set to anything other than [OFF].

6. Recording status (card slot 1)

   Displays the recording status of the SD card in the card slot 1.

   - : Not target for recording.

   - (flashing): Recognizing the SD card.

   - : The recording is stopped with the recording target SD card is inserted.

   - (flashing): Recognizing the SD card.

   - : Recording.

   - (Flashing red dot): Processing to stop the recording.

   - [P]: Recording is stopped with the pre-recording is enabled and the recording target SD card is inserted.

   - [P]: Pre-recording is enabled, and the SD card is not inserted in the card slot, or the SD card is not recognized.

   - (No display): It is in one of the following conditions.

     - The SD card is not inserted.

     - The SD card cannot be recognized.

     - The [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF], and recording is stopped.

   - : It is in one of the following conditions.

     - The [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF], and it is recording.

     - The tally lamp is instructed to illuminate in red via network.

7. Remaining recordable capacity and status of the SD card (card slot 1)

   Displays the remaining recordable capacity of the SD card and status of the SD card in the card slot 1.

   - [0min] to [999min]: Remaining recordable capacity (999 minutes or more is displayed as [999min])

     - The display will flash when the remaining recordable capacity becomes two minutes or less.

     - During the simultaneous recording, the remaining recordable capacity to be able to perform simultaneous recording (the one with smaller remaining recordable capacity of the two SD cards) is displayed.

   - [WP]: Write protected (the write protection switch on the SD card is at the LOCK side)

   - [END]: No remaining recordable capacity (there is no remaining recordable capacity in the SD card)

   - [ERR]: The SD card that cannot be recorded is inserted (it is recognized, but cannot be used such as format error, other than SD card, etc.)

   - [!SDXC]: The SDXC memory card is not inserted for MOV recording

   - (No display): It is in one of the following conditions.

     - The SD card is not inserted.

     - The SD card cannot be recognized.

     - The [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF].

8. Recording status (card slot 2)

   Displays the recording status of the SD card in the card slot 2.

   - : Not target for recording.

   - (flashing): Recognizing the SD card.

   - : The recording is stopped with the recording target SD card is inserted.

   - (flashing): Recognizing the SD card.

   - : Recording.

   - (Flashing red dot): Processing to stop the recording.

   - [P]: Recording is stopped with the pre-recording is enabled and the recording target SD card is inserted.

   - [P]: Pre-recording is enabled, and the SD card is not inserted in the card slot, or the SD card is not recognized.

   - (No display): It is in one of the following conditions.

     - The SD card is not inserted.

     - The SD card cannot be recognized.

     - The [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF].

9. Remaining recordable capacity and status of the SD card (card slot 2)

   Displays the remaining recordable capacity of the SD card and status of the SD card in the card slot 2.

   - [0min] to [999min]: Remaining recordable capacity (999 minutes or more is displayed as [999min])

     - The display will flash when the remaining recordable capacity becomes two minutes or less.

     - During the simultaneous recording, the remaining recordable capacity to be able to perform simultaneous recording (the one with smaller remaining recordable capacity of the two SD cards) is displayed.

   - [WP]: Write protected (the write protection switch on the SD card is at the LOCK side)

   - [END]: No remaining recordable capacity (there is no remaining recordable capacity in the SD card)

   - [ERR]: The SD card that cannot be recorded is inserted (it is recognized, but cannot be used such as format error, other than SD card, etc.)

   - [!SDXC]: The SDXC memory card is not inserted for MOV recording

   - (No display): It is in one of the following conditions.

     - The SD card is not inserted.

     - The SD card cannot be recognized.

     - The [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF].

10. Two-slot function

    Displays the setting status of the recording function using two SD cards.

    It is displayed with a slanted line if it is in a condition that cannot perform two-slot recording even if each function is enabled.

    - [RELAY]: When relay recording is enabled

    - [SIMUL]: When simultaneous recording is enabled

    - (No display): When it is standard recording

11. Time code

    Displays the time code, user bits, and duration in accordance with the [REC SETTINGS] menu → [TC] → [TC/UB/Dur.] setting.

    - [TC :::]: Displays the time code. (Displayed black and white inverted when slave locked to the externally input time code)

    - [UB ]: Displays the user bits.

    - [Dur :::]: Displays the duration.

12. Power supply status

    : Indicates the remaining battery level while powered with the battery. (The battery status display will change as → → → → while the remaining battery level gets lower. It will flash in red when the remaining battery level is zero)

    : Displays when powered with the AC adaptor.

13. Audio level meter

    Displays the volume.

    Displays the reference level position set in the [AUDIO SETTINGS] menu → [AUDIO CH SETTINGS] → [HEAD ROOM] → [18dB]/[20dB] is blacked out. (Eighth from left when set to [20dB], ninth from left when set to [18dB])

    - : Displays when audio cannot be recorded. (Such as when the variable frame rate recording function is enabled, and the frame rate is set different from the system frequency.)

14. Frame rate

    Displays the frame rate.

    Displays two places of decimals only when the frame rate is the same as the system frequency setting.

    This is not displayed when the system frequency is 60i/50i.

15. Shutter speed

    Displays the shutter speed.

    Display of [sec] and [deg] can be switched with the [CAMERA SETTINGS] menu → [SHUTTER] → [MODE]. Displays in time (minutes) display when set to [sec], and in aperture angle when set to [deg].

    Does not display when the shutter is disabled.

16. EXPOSURE INDEX

    Displays the sensitivity of the video. Display of [ISO] and [dB] can be switched with the [CAMERA SETTINGS] menu → [EI] → [MODE].

17. Spot meter

    Displays the brightness of the center in either [STOP] or [%] unit.

    When [V-Log] is selected, [STOP] and [%] can be switched with the [OUTPUT SETTINGS] menu → [LCD EI ASSIST] → [SPOT METER UNIT]. When anything other than [V-Log] is selected, the display is fixed as [%].

18. Color temperature

    Displays the selected color temperature.

    - [AK+.]: Displays the value of the color temperature and the setting value of GMg. [A] is displayed when the adjustment value acquired by the auto white balance is [AWB MEMORY A]. [B] is displayed when the adjustment value is [AWB MEMORY B].

    - [ATW]: Displays when the auto tracking white balance is operating.

    - [ATW LOCK]: Displays when the auto tracking white balance is locked.

19. Iris

    Displays the F value. ([A] is displayed when auto iris is operating)

    This is not displayed in the following cases.

    - When the lens is not connected

    - When the data cannot be acquired

20. Focus

    Displays the focus value.

    Display of the focus value follows the [OUTPUT SETTINGS] menu → [SDI/HDMI INDICATOR] → [FOCUS] and [OUTPUT SETTINGS] menu → [LCD INDICATOR] → [FOCUS] settings.

    Displays in feet/inch unit when set to [feet].

    Displays in meter unit when set to [m].

    This is not displayed in the following cases.

    - When the lens is not connected

    - When the data cannot be acquired

21. Zoom

    Displays the zoom distance in millimeter unit.

    This is not displayed in the following cases.

    - When the lens is not connected

    - When the data cannot be acquired

22. ND filter

    Displays the selected ND filter.

    - [ND:1.8]: Reduces the amount of light entering the MOS sensor to 1/64.

    - [ND:1.2]: Reduces the amount of light entering the MOS sensor to 1/16.

    - [ND:0.6]: Reduces the amount of light entering the MOS sensor to 1/4.

    - [ND:CLR]: The ND filter is not used.

23. Special recording function

    Displays the status of special recording function.

    - [INTRVL]: The interval recording is stopped.

    - [I-REC]: The interval recording is in progress. (Displayed in red)

24. Message display area

    Displays the message such as the camera status or the warning.

25. Level gauge

    Tilt in horizontal direction or vertical direction can be checked.

    Displays only on the LCD monitor.

26. Wireless LAN connection status

    Displays the connection status of the wireless LAN.

27. External equipment recording operation control status (<SDI OUT>/<HDMI> terminal)

    Displays the control status of the recording start and recording stop on the external equipment connected to the <SDI OUT> terminal and the <HDMI> terminal.

    - [S/H]: Recording instruction is output to the output from the <SDI OUT> terminal, <HDMI> terminal.

    - [S/H]: Pause instruction is output to the output from the <SDI OUT> terminal, <HDMI> terminal.

    - [SDI]: Recording instruction is output to the output from the <SDI OUT> terminal.

    - [SDI]: Pause instruction is output to the output from the <SDI OUT> terminal.

    - [HDMI]: Recording instruction is output to the output from the <HDMI> terminal.

    - [HDMI]: Pause instruction is output to the output from the <HDMI> terminal.

28. Waveform monitor

    Displays the video status in waveform or vector.

    Displays only on the LCD monitor.

29. IR shooting

    Displays when the IR recording is set to enable.

30. Electronic image stabilization function/digital zoom

    Displays when the electronic image stabilization function is set or the digital zoom is enabled.

    - [EIS]: Displays when the electronic image stabilization function is enabled.

    - [D1.4x]: Displays when the 1.4x digital zoom is enabled.

#### During playback

1. Playback status

   Displays the status of playback.

   Displays only during playback.

   - : Stop

   - : Playback

   - : Pause

   - : Frame-by-frame rewind

   - : Frame-by-frame

   - : Fast-forward playback (10x speed)

   - : Fast-forward playback (20x speed)

   - : Fast-reverse playback (10x speed)

   - : Fast-reverse playback (20x speed)

   - : Slow playback

   - : Reverse slow playback

2. Direct playback bar

   Displays the general position that is being played back.

3. Playback navigation button

   Operates by touching the button.

   - : Fast-forward playback

   - : Fast-reverse playback

   - : Stop

   - /: Playback/pause

4. Still picture record button

   If a scene is selected by touching this button or pressing the multidial while playing back or pausing the playback, the scene is recorded as a still picture.

Top of the page