- Top
- Preparation
- Mounting accessories
- LCD monitor unit

# LCD monitor unit

## Mounting the LCD monitor unit

Mount the supplied LCD monitor unit to the LCD monitor mounting section.

Screw

Fig. 1

Fig. 2

Fig. 3

Insert the supplied LCD monitor mounting attachment to the LCD monitor unit mounting section of the handle. (Fig. 1)

- This can also be mounted to the accessory mounting holes at the top of the camera.

Tighten the supplied screw by turning clockwise.

Open the terminal cover of the <LCD> terminal, and connect the LCD monitor unit cable to the <LCD> terminal. (Fig. 2)

- Connect by aligning of the <LCD> terminal with of the LCD monitor unit cable connection terminal.

- Connect after confirming that of the LCD monitor unit cable connection terminal is facing outward.

Attach the LCD monitor unit cable to the LCD monitor cable clamp. (Fig. 3)

#### Adjusting the angle of the LCD monitor

The LCD monitor can be turned vertically and horizontally to adjust to easily viewable angle.

The VIEW screen can be inverted vertically or inverted vertically and horizontally by the <MIRROR> switch allowing the mirror shooting, etc.

It is recommended to close the LCD monitor to protect the LCD monitor when the camera is not used or to be carried.

## Removing the LCD monitor unit

Remove in the reverse procedure as mounting.

NOTE

- To disconnect the LCD monitor unit cable, pull out while pressing on the lock buttons on both sides of the cable connection terminal ().

## LCD monitor hood

The LCD monitor hood is already mounted to the LCD monitor unit.

### Removing the LCD monitor hood

Remove the LCD monitor hood while pushing in your nails into the gaps of the tabs (2 locations) at the upper of the LCD monitor hood.

The LCD monitor hood is removed.

### Opening and closing of the LCD monitor hood

NOTE

- Close the LCD monitor hood to protect the LCD monitor when the LCD monitor unit is not used.

### Mounting the LCD monitor hood

Align the tabs at the top of the LCD monitor hood (2 locations) to the dimples at the top of the LCD monitor unit.

Align the tabs at the bottom of the LCD monitor hood (2 locations) to the dimples at the bottom of the LCD monitor unit.

Top of the page