- Top
- Shooting
- Shooting
- Selecting the resolution and frame rate of the RAW output

# Selecting the resolution and frame rate of the RAW output

Resolution of the RAW output from the <SDI OUT> terminal can be selected in the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW].

When [SDI RAW] is set to anything other than [OFF], [SENSOR MODE], [MAIN PIXEL], and [MAIN CODEC] cannot be set.

[FREQUENCY] | [SDI RAW] | VFR
--- | --- | ---
[23.98p] [24.00p] [29.97p] | [S35 5.7K] | 1fps - 30fps
[CROP 4K] | 1fps - 60fps
[CROP&MIX 2K] | 1fps - 240fps
[25.00p] | [S35 5.7K] | 1fps - 25fps
[CROP 4K] | 1fps - 50fps
[CROP&MIX 2K] | 1fps - 200fps
[50.00p] | [CROP 4K] | 1fps - 50fps
[CROP&MIX 2K] | 1fps - 200fps
[59.94p] | [CROP 4K] | 1fps - 60fps
[CROP&MIX 2K] | 1fps - 240fps

NOTE

- When [FREQUENCY] is set to [50.00i]/[59.94i], [SDI RAW] is fixed to [OFF].

Top of the page