- Top
- Connecting to External Devices
- Connecting the camera and the iPad/Android terminal
- Direct connection ([DIRECT])

# Direct connection ([DIRECT])

This is the setting to connect the camera to the iPad/Android terminal directly.

The camera may restart if necessary when the setting is changed.

Select the [NETWORK SETTINGS] menu → [NETWORK PROPERTY] → [TYPE] → [DIRECT].

From the [NETWORK SETTINGS] menu → [NETWORK PROPERTY], set each item as necessary.

- For details of setting, refer to “Setting items in [NETWORK PROPERTY] when set to [DIRECT]”.

Select the [NETWORK SETTINGS] menu → [NETWORK SEL] → [WLAN].

Select the SSID of the camera from the SSID list in the iPad/Android terminal, and enter the password (encryption key).

Display the wireless access point list screen in wireless LAN setting, and select SSID of the camera.

- Factory setting: [AU-EVA1]

When the password confirmation screen appears, enter the password (encryption key).

- Factory setting: [01234567890123456789abcdef]

Check the network connection.

Once connected, is displayed on the screen of the camera.

#### Setting items in [NETWORK PROPERTY] when set to [DIRECT]

[SSID] | Network name of the camera (SSID) (Factory setting: [AU-EVA1])
[BAND] | Setting to switch between two communication method ([2.4GHz] or [5GHz]) (Factory setting: [2.4GHz])
[CHANNEL(2.4GHz)] | Channel to be used when [BAND] is set to [2.4GHz] (Factory setting: [AUTO])
[CHANNEL(5GHz)] | Channel to be used when [BAND] is set to [5GHz] (Factory setting: [AUTO])
[ENCRYPT KEY] | WPA2 encryption key (Factory setting: [01234567890123456789abcdef])
[DHCP] | Setting the DHCP function [OFF]: Does not use the DHCP function. [CLIENT]: When connecting by setting [TYPE] to [INFRA(SELECT)] or [INFRA(MANUAL)], it is acquired automatically from the DHCP. (Cannot be selected.) [SERVER]: Enables the DHCP server function of the camera when connecting with [TYPE] set to [DIRECT]. (Factory setting: [SERVER])
[IP ADDRESS] | IP address of the camera (Factory setting: [192.168.0.1])
[SUBNET MASK] | Subnet mask (Factory setting: [255.255.255.0])
[DEFAULT GATEWAY] | Default gateway (Factory setting: [192.168.0.254])

NOTE

- [DHCP] will be set to [SERVER].

- [ENCRYPTION] will be fixed to [WPA2-AES].

- Depending on the used wireless module, some of the items in [BAND], [CHANNEL(2.4GHz)], and [CHANNEL(5GHz)] may not be able to select.

Top of the page