- Top
- Output and Screen Display
- Output format
- Format that can be output from the <HDMI> terminal

# Format that can be output from the <HDMI> terminal

The format that can be output from the <HDMI> terminal differs with following combination of the settings.

- The [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [FREQUENCY]

- The [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [MAIN PIXEL]

- The [OUTPUT SETTINGS] menu → [HDMI OUT] → [SIGNAL SEL]

- The [OUTPUT SETTINGS] menu → [HDMI OUT] → [OUT FORMAT]

Item | Output Format [OUT FORMAT]
--- | ---
[FREQUENCY] | [MAIN PIXEL] | [SIGNAL SEL]
[59.94p] [50.00p] | [4096×2160] | [HDMI] | 4096×2160p 4096×2160p (4:2:0/8 bits) 1920×1080p*1 (Factory setting) 1920×1080i*1
|  | [LCD(1080p)] | 1920×1080p*2
| [3840×2160] | [HDMI] | 3840×2160p 3840×2160p (4:2:0/8 bits) 1920×1080p (Factory setting) 1920×1080i
|  | [LCD(1080p)] | 1920×1080p*2
| [2048×1080] | [HDMI] | 1920×1080p*1 (Factory setting) 1920×1080i*1
|  | [LCD(1080p)] | 1920×1080p*2
| [1920×1080] | [HDMI] | 1920×1080p (Factory setting) 1920×1080i
|  | [LCD(1080p)] | 1920×1080p*2
| [1280×720] | [HDMI] | 1280×720p (Factory setting)
|  | [LCD(1080p)] | 1920×1080p*2
[59.94i] [50.00i] | [1920×1080] | [HDMI] | 1920×1080i (Factory setting) 720×480p (when [59.94i]) 720×576p (when [50.00i])
|  | [LCD(1080p)] | 1920×1080p*2
[29.97p] [23.98p] | [4096×2160] | [HDMI] | 4096×2160p 1920×1080p*1 (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 59.94p*2
| [3840×2160] | [HDMI] | 3840×2160p 1920×1080p (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 59.94p*2
| [2048×1080] | [HDMI] | 1920×1080p*1 (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 59.94p*2
| [1920×1080] | [HDMI] | 1920×1080p (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 59.94p*2
[24.00p] | [4096×2160] | [HDMI] | 4096×2160p 1920×1080p*1 (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 60p*2
| [2048×1080] | [HDMI] | 1920×1080p*1 (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 60p*2
[25.00p] | [4096×2160] | [HDMI] | 4096×2160p 1920×1080p*1 (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 50p*2
| [3840×2160] | [HDMI] | 3840×2160p 1920×1080p (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 50p*2
| [2048×1080] | [HDMI] | 1920×1080p*1 (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 50p*2
| [1920×1080] | [HDMI] | 1920×1080p (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 50p*2

Displayed in the letterbox format. Quality is slightly lower compared to recorded image.

It will be the same image as the LCD monitor with black band in all four sides. Focus and EI assist display are possible. Equivalent to 4:2:2 (8 bits). The time code information is not output.

Following functions are not displayed.

Focus square display

Waveform monitor

Zebra pattern when the skin tone detail function is set to enable

NOTE

- The output will be as follows regardless of [FREQUENCY] or [MAIN PIXEL] when [SIGNAL SEL] is set to [LCD(1080p)].

  - When [FREQUENCY] is set to [59.94p]/[59.94i]/[29.97p]/[23.98p]: 1920×1080 over 59.94p

  - When [FREQUENCY] is set to [50.00p]/[50.00i]/[25.00p]: 1920×1080 over 50p

  - When [FREQUENCY] is set to [24.00p]: 1920×1080 over 60p

- The 2048×1080 output is not supported.

- [OUT FORMAT] will change to the factory setting when the settings of [FREQUENCY] and [MAIN PIXEL] change and current settings in [OUT FORMAT] cannot be acquired.

- The output format when playing back from the thumbnail screen is as follows.

  - It will be the value set in [OUT FORMAT] when the recording resolution of the playback clip is the same as [MAIN PIXEL].

  - It will be factory setting of [OUT FORMAT] when the recording resolution of the playback clip is different from [MAIN PIXEL].

- When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF], and the [OUTPUT SETTINGS] menu → [HDMI OUT] → [SIGNAL SEL] is set to [HDMI], [OUT FORMAT] is fixed to [1920×1080p].

- When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF], the time code information is not output.

Top of the page