- Top
- Operation
- Displaying the HOME screen

# Displaying the HOME screen

Status of the camera can be confirmed.

1. [FPS]

   Displays the setting status of the variable frame rate recording function and the recording frame rate.

2. [COLOR]

   Displays the color setting of the video recorded to the main recorder.

3. [SHUTTER]

   Displays the shutter speed.

   [sec]: Displays in time.

   [deg]: Displays at shutter open angle.

4. [EI]

   Displays the EXPOSURE INDEX (gain).

   [ISO] and [dB] can be switched with the [CAMERA SETTINGS] menu → [EI] → [MODE].

5. [AUDIO]

   Displays the status of the audio input for audio channel 1 and the audio channel 2.

   [IN1]: The <AUDIO INPUT 1> terminal is selected as the audio input.

   [IN2]: The <AUDIO INPUT 2> terminal is selected as the audio input.

   [MIC]: An external microphone is selected as the audio input.

   [LINE]: An audio device is selected as the audio input.

   [INT(L)]: The built-in microphone <L> is selected as the audio input.

   [INT(R)]: The built-in microphone <R> is selected as the audio input.

   [48V]: The external microphone power supply is enabled.

6. [WB]

   Displays the color temperature (white balance).

   When the adjusted value acquired by the auto white balance is [AWB MEMORY A], the color temperature is displayed with [A] at the beginning. When the adjusted value acquired by the auto white balance is [AWB MEMORY B], the color temperature is displayed with [B] at the beginning.

   [ATW]: Displays while the auto tracking white balance is operating.

   [ATW LOCK]: Displays when the auto tracking white balance is locked.

7. Number of recorded pixels/system frequency

   Displays the number of recording pixels and the system frequency.

   When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF], the RAW output resolution and the system frequency from <SDI OUT> terminal are displayed.

8. Pre-recording status display

   Displays the re-recording status.

   : When the [REC SETTINGS] menu → [PRE REC] → [ON] is set and pre-recording is enabled

   (No display): When the [REC SETTINGS] menu → [PRE REC] → [OFF] is set, or when pre-recording is unable

9. Card slot 1/card slot 2 status display

   Indicates the insertion status, current recording target, and remaining recordable capacity of the SD card.

   : When the SD card is inserted, and it is set as the recording target

   : When the SD card is inserted, but it is not set as the recording target

   [0min]…[999min]: Remaining recordable capacity (0 - 999 minutes, 999 minutes or more is displayed as [999min])

   [END]: When there is no remaining recordable capacity

   [WP]: When the write protect switch of the SD card is set to the LOCK side

   [!SDXC]: When the SDHC memory card is inserted, and the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [MAIN CODEC] is set to a file in MOV format (displayed in red)

   [ERR]: When a recording media that cannot be recorded is inserted (displayed in red)

   (No display): When the SD card is not inserted, or when the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF]

10. Special recording function display

    Displays the setting and enable/disable status of the special recording function of each card slot.

    [RELAY]: When set to relay recording

    [SIMUL]: When set to simultaneous recording

    [INTRVL]: When set to interval recording

11. Wireless LAN connection status display

    Displays the connection status of the wireless LAN.

    (No display): When the [NETWORK SETTINGS] menu → [NETWORK SEL] → [OFF] is set

    : When ROP is not connected

    : When ROP is connected

12. Power status display

    Displays the remaining battery level, or the drive status of the AC adaptor.

    : Driving with the battery (remaining battery level)

    : Driving with the AC adaptor

13. Main recording codec

    Displays the recording codec of the main recorder.

    [ONLY SDI RAW]: When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF]

14. Warning/alert display (Cases indicated by error messages)

    : Warning display

    : Alert display

15. Time code display

    [TCG :::]: Displays the value of the time code generator

    [UBG ]: Displays the value of the user bits generator

    [Dur. :::]: Displays the value of the duration

16. Audio level meter

    Displays the recording level of audio with 18 bars. (2 dB steps)

    Displays in red bar when exceeding 0 dB.

    : During a mode that cannot record audio such as when the variable frame rate recording function is enabled and the set frame rate is different from the system frequency

17. External output terminal output image setting display

    Displays the output image of the external output terminal set in the [SYSTEM SETTINGS] menu → [COLOR SETTINGS] → [SDI OUT]/[HDMI OUT]/[LCD OUT].

    The output image of the external output terminal set in following menu is displayed when set to the [SYSTEM SETTINGS] menu → [COLOR SETTINGS] → [MAIN] → [SCENE1] to [SCENE5] and the [SCENE FILE SETTINGS] menu → [GAMMA] → [GAMMA SELECT] → [HLG].

    - [OUTPUT SETTINGS] menu → [SDI OUT] → [SDI OUT HDR]

    - [OUTPUT SETTINGS] menu → [HDMI OUT] → [HDMI OUT HDR]

    - [OUTPUT SETTINGS] menu → [LCD HDR]

    When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF], [RAW] is displayed in [SDI].

18. CAM INDEX/REEL COUNT

    Displays the CAM INDEX, REEL COUNT, and clip number. Information about last recorded clip is displayed.

    : CAM INDEX and REEL COUNT (A001 to Z999)

    : Clip number (C001 to C999)

Top of the page