- Top
- Specification
- Specifications
- Battery charger (AG-BRD50)

# Battery charger (AG-BRD50)

Input voltage DC 12 V, 3.0 A Output voltage DC 8.4 V, 4.0 A

indicates safety information.

Charging current | Maximum 4,000 mA
Operating ambient humidity | 10% - 80% (relative humidity, no condensation)
Mass | Approx. 230 g (0.507 lbs.)
Dimensions (W×H×D) | 130 mm×48 mm×107 mm (5-1/8 inches×1-7/8 inches×4-3/16 inches)

Top of the page