- Top
- Operation
- Menu setting contents
- [SYSTEM SETTINGS] menu

# [SYSTEM SETTINGS] menu

Sets the system in general.

## [SYSTEM MODE]

For the combination that can be set, refer to “Selecting the resolution, codec, and frame rate for recording video”, “Selecting the resolution and frame rate of the RAW output”.

### [FREQUENCY]

Sets the system frequency.

The items that can be set are as follows.

- [23.98p], [24.00p], [25.00p], [29.97p], [50.00p], [59.94p], [50.00i], [59.94i]

(Factory setting: [23.98p])

NOTE

- The camera will restart when the setting is changed.

- When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [MAIN CODEC] is set to AVCHD format, different clips with system frequency in 59.94 Hz system (23.98p, 59.94p, 59.94i) and the ones in 50 Hz system (50.00p, 50.00i) cannot be recorded in a single SD card. Prepare an SD card for each system of system frequency (59.94 Hz system and 50 Hz system). [FORMAT ERROR CARD <SLOT 1>]/[FORMAT ERROR CARD <SLOT 2>] alert is displayed when the system frequency systems are different.

### [SDI RAW]

Sets the RAW output resolution from the <SDI OUT> terminal.

[OFF] | Does not perform RAW output.
[S35 5.7K] | Performs the RAW output of the 5760×3072 pixels using all the pixels of the image sensor. Allows shooting up to 30p.
[CROP 4K] | Performs the RAW output of the 4096×2160 pixels by cutting out the center section of the image sensor. Allows shooting up to 60p. Angle of view will change.
[CROP&MIX 2K] | Performs the RAW output of the 2048×1080 pixels by cutting out the center section of the image sensor and performing the pixel mixing read. This allows high-speed shooting up to 240p. Angle of view will change.

(Factory setting: [OFF])

NOTE

- When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [FREQUENCY] is set to [50.00i]/[59.94i], this is fixed to [OFF].

- When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [FREQUENCY] is set to [50.00p]/[59.94p], [S35 5.7K] cannot be selected.

- Following conditions apply when set to anything other than [OFF].

  - Recording to an SD card with the camera is not possible.

  - The [SYSTEM SETTINGS] menu → [COLOR SETTINGS] → [MAIN] will be fixed to [V-Log].

  - The [CAMERA SETTINGS] menu → [EI] → [MODE] will be fixed to [ISO].

  - The thumbnail screen is not displayed.

  - [E.I.S.], [D.ZOOM], [PRE REC], [REC CHECK], [DEL LAST CLIP], [SLOT SEL], [SDI COLOR], and [COLOR BARS] assigned to the USER button will not operate.

  - The [OUTPUT SETTINGS] menu → [SDI OUT] → [SDI REC REMOTE] and the [OUTPUT SETTINGS] menu → [HDMI OUT] → [HDMI REC REMOTE] will not operate.

  - The time code information is not output in the image output from the <HDMI> terminal.

### [SENSOR MODE]

Sets the drive mode of the image sensor.

[S35 5.7K] | Uses the entire pixels of the image sensor.
[S35 MIX 2.8K] | Performs pixel mixing read of 2.8K from the entire image sensor. This allows high-speed shooting up to 120p.
[4/3 CROP&MIX 2.2K] | Performs the pixel mixing read of 2.2K by cropping the Four Thirds image circle from the center of the image sensor. This allows high-speed shooting up to 240p. Angle of view will change.

(Factory setting: [S35 5.7K])

NOTE

- When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SENSOR MODE] → [4/3 CROP&MIX 2.2K] is set

  - The sensitivity will be lower than when [S35 5.7K] or [S35 MIX 2.8K] is set.

  - The items that can be set in the [CAMERA SETTINGS] menu → [EI] → [NATIVE ISO] will be [400 ISO] or [1250 ISO].

- When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF], this cannot be set.

### [MAIN PIXEL]

Sets the main recorder’s number of recording pixels.

The items that can be set are as follows.

- [4096×2160], [3840×2160], [2048×1080], [1920×1080], [1280×720]

(Factory setting: [4096×2160])

NOTE

- When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF], this cannot be set.

### [MAIN CODEC]

Sets the recording codec of the main recorder.

- MOV file

  [HEVC LongGOP 200M] | 4:2:0 (10 bits) LongGOP 200 Mbps
  [HEVC LongGOP 150M] | 4:2:0 (10 bits) LongGOP 150 Mbps
  [420LongGOP 150M] | 4:2:0 (8 bits) LongGOP 150 Mbps
  [420LongGOP 100M] | 4:2:0 (8 bits) LongGOP 100 Mbps
  [420LongGOP 50M] | 4:2:0 (8 bits) LongGOP 50 Mbps
  [422LongGOP 150M] | 4:2:2 (10 bits) LongGOP 150 Mbps
  [422LongGOP 100M] | 4:2:2 (10 bits) LongGOP 100 Mbps
  [422LongGOP 50M] | 4:2:2 (10 bits) LongGOP 50 Mbps
  [422ALL-I 400M] | 4:2:2 (10 bits) ALL-Intra 400 Mbps
  [422ALL-I 200M] | 4:2:2 (10 bits) ALL-Intra 200 Mbps
  [422ALL-I 100M] | 4:2:2 (10 bits) ALL-Intra 100 Mbps

- AVCHD file

  [AVCHD PS] | 4:2:0 (8 bits) LongGOP 25 Mbps
  [AVCHD PH] | 4:2:0 (8 bits) LongGOP 21 Mbps
  [AVCHD HA] | 4:2:0 (8 bits) LongGOP 17 Mbps
  [AVCHD PM] | 4:2:0 (8 bits) LongGOP 8 Mbps

(Factory setting: [422LongGOP 150M])

NOTE

- When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF], this cannot be set.

## [COLOR SETTINGS]

### [MAIN]

Sets the colors of videos (entire camera system) recorded in the main recorder.

[V-Log] | Sets to the gamma curve that can achieve gradation and wide latitude (exposure range). A grading process after recording is required.
[SCENE1], [SCENE2], [SCENE3], [SCENE4], [SCENE5] | Sets to setting to perform detailed image quality adjustment with the camera. When [SCENE1] to [SCENE5] is selected, the menu setting for the same scene number is enabled in the [SCENE FILE SETTINGS] menu.

(Factory setting: [V-Log])

NOTE

- When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF], this will be fixed to [V-Log].

### [SDI OUT]

Sets the output image from the <SDI OUT> terminal.

- When [MAIN] in [COLOR SETTINGS] is set to [V-Log]

[V-Log] | Outputs with the same color as the video recorded in the main recorder.
[V-709] | Outputs by converting to a color comparable to the standard CINE-LIKE. This is the setting appropriate for preview.

- When [MAIN] in [COLOR SETTINGS] is set to [SCENE1], [SCENE2], [SCENE3], [SCENE4], or [SCENE5]

[SCENE1], [SCENE2], [SCENE3], [SCENE4], [SCENE5] | Outputs with the same color as the video recorded in the main recorder. This cannot be changed.

(Factory setting: [V-Log])

NOTE

- When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF], this will be fixed to [V-Log].

### [HDMI OUT]

Sets the output image from the <HDMI> terminal.

- When [MAIN] in [COLOR SETTINGS] is set to [V-Log]

[V-Log] | Outputs with the same color as the video recorded in the main recorder.
[V-709] | Outputs by converting to a color comparable to the standard CINE-LIKE. This is the setting appropriate for preview.

- When [MAIN] in [COLOR SETTINGS] is set to [SCENE1], [SCENE2], [SCENE3], [SCENE4], or [SCENE5]

[SCENE1], [SCENE2], [SCENE3], [SCENE4], [SCENE5] | Outputs with the same color as the video recorded in the main recorder. This cannot be changed.

(Factory setting: [V-Log])

### [LCD OUT]

Sets the output image from the <LCD> terminal.

- When [MAIN] in [COLOR SETTINGS] is set to [V-Log]

[V-Log] | Outputs with the same color as the video recorded in the main recorder.
[V-709] | Outputs by converting to a color comparable to the standard CINE-LIKE. This is the setting appropriate for preview.

- When [MAIN] in [COLOR SETTINGS] is set to [SCENE1], [SCENE2], [SCENE3], [SCENE4], or [SCENE5]

[SCENE1], [SCENE2], [SCENE3], [SCENE4], [SCENE5] | Outputs with the same color as the video recorded in the main recorder. This cannot be changed.

(Factory setting: [V-Log])

## [USER SWITCHES]

The function to assign the <USER 1> to <USER 9> buttons and multidial can be set.

For details, refer to “Assigning function to the USER buttons”.

Following functions can be assigned to [USER1] to [USER9].

- [INHIBIT], [AWB], [ONE PUSH AF], [ONE PUSH A.IRIS], [ATW LOCK], [E.I.S.], [D.ZOOM], [IR SHOOTING], [REC SW], [PRE REC], [VFR], [REC CHECK], [DEL LAST CLIP], [SLOT SEL], [EXPAND], [OPEN IRIS F.A.], [PEAK./SQUARES F.A.], [WFM], [SPOT METER], [ZEBRA], [LEVEL GAUGE], [LEVEL GAUGE SET], [SDI COLOR], [HDMI COLOR], [LCD COLOR], [SDI OUT HDR], [HDMI OUT HDR], [LCD HDR], [LCD CLEAN VIEW], [LCD MARKER], [COLOR BARS], [LOAD SETUP FILE], [POWER LCD]

[USER1] | Sets the function to assign to the <USER 1> button. (Factory setting: [ONE PUSH AF])
[USER2] | Sets the function to assign to the <USER 2> button. Assigned function is enabled when the VIEW screen is displayed. (Factory setting: [PEAK./SQUARES F.A.])
[USER3] | Sets the function to assign to the <USER 3> button. Assigned function is enabled when the VIEW screen is displayed. (Factory setting: [SPOT METER])
[USER4] | Sets the function to assign to the <USER 4> button. (Factory setting: [E.I.S.])
[USER5] | Sets the function to assign to the <USER 5> button. (Factory setting: [WFM])
[USER6] | Sets the function to assign to the <USER 6> button. (Factory setting: [AWB])
[USER7] | Sets the function to assign to the <USER 7> button. (Factory setting: [SLOT SEL])
[USER8] | Sets the function to assign to the <USER 8> button. (Factory setting: [EXPAND])
[USER9] | Sets the function to assign to the <USER 9> button. (Factory setting: [OPEN IRIS F.A.])
[USER TOGGLE] | Sets the function to assign to the multidial. Assigned function is enabled when the VIEW screen is displayed. The items that can be set are as follows. [INHIBIT], [SHUTTER], [FPS], [MONITOR VOL] (Factory setting: [MONITOR VOL])

## [SIDE LOCK]

### [REC]

Sets if the REC button is to be locked or not with the <LOCK> switch.

[LOCK] | It will be locked.
[UNLOCK] | It will not be locked.

(Factory setting: [UNLOCK])

### [USER1]

Sets if the <USER 1> button is to be locked or not with the <LOCK> switch.

[LOCK] | It will be locked.
[UNLOCK] | It will not be locked.

(Factory setting: [LOCK])

### [USER2]

Sets if the <USER 2> button is to be locked or not with the <LOCK> switch.

[LOCK] | It will be locked.
[UNLOCK] | It will not be locked.

(Factory setting: [LOCK])

### [USER3]

Sets if the <USER 3> button is to be locked or not with the <LOCK> switch.

[LOCK] | It will be locked.
[UNLOCK] | It will not be locked.

(Factory setting: [LOCK])

### [USER4]

Sets if the <USER 4> button is to be locked or not with the <LOCK> switch.

[LOCK] | It will be locked.
[UNLOCK] | It will not be locked.

(Factory setting: [LOCK])

### [USER5]

Sets if the <USER 5> button is to be locked or not with the <LOCK> switch.

[LOCK] | It will be locked.
[UNLOCK] | It will not be locked.

(Factory setting: [LOCK])

### [USER6]

Sets if the <USER 6> button is to be locked or not with the <LOCK> switch.

[LOCK] | It will be locked.
[UNLOCK] | It will not be locked.

(Factory setting: [LOCK])

### [USER7]

Sets if the <USER 7> button is to be locked or not with the <LOCK> switch.

[LOCK] | It will be locked.
[UNLOCK] | It will not be locked.

(Factory setting: [LOCK])

### [THUMBNAIL]

Sets if the <THUMBNAIL> button is to be locked or not with the <LOCK> switch.

[LOCK] | It will be locked.
[UNLOCK] | It will not be locked.

(Factory setting: [LOCK])

### [HOME]

Sets if the <HOME> button is to be locked or not with the <LOCK> switch.

[LOCK] | It will be locked.
[UNLOCK] | It will not be locked.

(Factory setting: [LOCK])

### [ND FILTER]

Sets if the <ND FILTER> button is to be locked or not with the <LOCK> switch.

[LOCK] | It will be locked.
[UNLOCK] | It will not be locked.

(Factory setting: [LOCK])

### [IRIS DIAL]

Sets if the <IRIS> button is to be locked or not with the <LOCK> switch.

[LOCK] | It will be locked.
[UNLOCK] | It will not be locked.

(Factory setting: [LOCK])

### [MENU]

Sets if the <MENU> button is to be locked or not with the <LOCK> switch.

[LOCK] | It will be locked.
[UNLOCK] | It will not be locked.

(Factory setting: [LOCK])

### [EXIT]

Sets if the <EXIT> button is to be locked or not with the <LOCK> switch.

[LOCK] | It will be locked.
[UNLOCK] | It will not be locked.

(Factory setting: [LOCK])

### [MULTI DIAL]

Sets if the multidial is to be locked or not with the <LOCK> switch.

[LOCK] | It will be locked.
[UNLOCK] | It will not be locked.

(Factory setting: [LOCK])

## [LED & FAN]

### [TALLY LED]

Sets if the tally lamp is to illuminate or not.

[FRONT] | The front tally lamp will illuminate.
[REAR] | The rear tally lamp will illuminate.
[BOTH] | Both the front and rear tally lamps will illuminate.
[OFF] | The tally lamp will not illuminate.

(Factory setting: [BOTH])

### [ACCESS LED]

Sets if the card access lamp is to illuminate or not.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

### [POWER LED]

Sets if the power lamp is to illuminate or not.

The items that can be set are as follows.

- [ON], [OFF]

(Factory setting: [ON])

NOTE

- It will illuminate approximately one second even if it is set to [OFF].

### [FAN SPEED]

Sets the rotation speed of the fan.

[AUTO] | It will rotate in slow speed until the specified temperature is reached, and then it will rotate in the same speed as [FULL] when the specified temperature is reached.
[FULL] | It will always rotate in constant speed.

(Factory setting: [AUTO])

## [LCD]

### [BRIGHTNESS]

Adjusts the brightness of the LCD monitor.

The items that can be set are as follows.

- [−15]…[15]

(Factory setting: [0])

### [COLOR LEVEL]

Adjusts the color level of the LCD monitor color.

The items that can be set are as follows.

- [−15]…[15]

(Factory setting: [0])

### [CONTRAST]

Adjusts the contrast of the LCD monitor.

The items that can be set are as follows.

- [−30]…[30]

(Factory setting: [0])

### [BACK LIGHT]

Adjusts the brightness of the LCD monitor backlight. [0] is the standard brightness.

When [POWER LCD] is assigned to the USER button and the function is enabled, the brightness will not change even when the setting of [BACK LIGHT] is changed.

The items that can be set are as follows.

- [−1], [0], [1]

(Factory setting: [0])

## [CLOCK]

### [CLOCK SETTING]

Sets the calendar (date of the built-in clock) and time.

[YEAR] | [2017]…[2037]
[MONTH] | [JAN]…[DEC] ([1]…[12])
[DAY] | [1]…[31] ([28], [29], [30])
[HOUR] | [0]…[23]
[MINUTE] | [0]…[59]

(Factory setting: [YEAR]: [2017], [MONTH]: [1], [DAY]: [1], [HOUR]: [0], [MINUTE]: [0])

### [TIME ZONE]

Sets the time zone. It will switch to the time with the time difference added when the time zone setting is changed.

The items that can be set are as follows.

- [−12:00]…[+12:30] (30 minutes steps), [+12:45], [+13:00]

(Factory setting: [+0:00])

### [DATE FORMAT]

Sets the display order of the year, month, and date of the calendar (date of the built-in clock). This is reflected to the date display of the clip information.

The items that can be set are as follows.

- [Y-M-D], [M-D-Y], [D-M-Y]

(Factory setting: [Y-M-D] (when [AREA SETTINGS] is set to [AREA 1]), [M-D-Y] (when [AREA SETTINGS] is set to [AREA 2]), [D-M-Y] (when [AREA SETTINGS] is set to [AREA 3]))

## [INFORMATION]

Displays the information of the camera.

[VERSION] | [MODEL] | Displays the product name of the camera.
[SERIAL NO.] | Displays the serial number of the camera.
[VERSION] | Displays the firmware version of the camera.
[OPERATION TIME] | [TOTAL OPERATION] | Displays the total operation time.
[IRIS DIAL] | Displays the total number of upward rotation or downward rotation of the <IRIS> dial by updating every time it reaches 100 turns. (“T” indicates the number.)
[SENSOR TEMP] | Displays the ambient temperature of the image sensor.
[USB SERVICE MODE] | Switches to the USB service mode.
[UPDATE] | Updates the firmware.

## [LANGUAGE]

Sets the display language.

This is not displayed when the [OPTION] menu → [AREA SETTINGS] → [AREA 1] is set.

This is displayed only when the [OPTION] menu → [AREA SETTINGS] → [AREA 2]/[AREA 3] is set.

[English] | English
[Español] | Spanish
[Français] | French

(Factory setting: [English])

## [INITIALIZE]

### [LOAD FACTORY DATA]

Returns the setting value of the menu to the factory setting. The camera is restarted after executing.

The items that can be selected are as follows.

- [YES], [NO]

Top of the page