- Top
- Shooting
- Shooting
- Selecting the resolution, codec, and frame rate for recording video

# Selecting the resolution, codec, and frame rate for recording video

The resolution, codec, and frame rate of the recording video can be selected in the [SYSTEM SETTINGS] menu → [SYSTEM MODE].

- [FREQUENCY]: System frequency

- [SDI RAW]: Resolution (RAW output resolution from the <SDI OUT> terminal)

  When [SDI RAW] is set to anything other than [OFF], [SENSOR MODE], [MAIN PIXEL], and [MAIN CODEC] cannot be set.

- [SENSOR MODE]: Drive mode of the sensor

- [MAIN PIXEL]: Resolution

- [MAIN CODEC]: Recording codec

  - 4:2:0 (10 bits) LongGOP MOV: [HEVC LongGOP 200M], [HEVC LongGOP 150M]

  - 4:2:0 (8 bits) LongGOP MOV: [420LongGOP 150M], [420LongGOP 100M], [420LongGOP 50M]

  - 4:2:2 (10 bits) LongGOP MOV: [422LongGOP 150M], [422LongGOP 100M], [422LongGOP 50M]

  - 4:2:2 (10 bits) ALL-Intra MOV: [422ALL-I 400M], [422ALL-I 200M], [422ALL-I 100M]

  - AVCHD: [AVCHD PS], [AVCHD PH], [AVCHD HA], [AVCHD PM]

- VFR: Variable frame rate recording function (variable frame rate range)

## When [FREQUENCY] is set to [23.98p]

Can be set only when [SDI RAW] is set to [OFF].

[SENSOR MODE] | [MAIN PIXEL] | [MAIN CODEC] | VFR
--- | --- | --- | ---
[S35 5.7K] | [4096×2160] | [HEVC LongGOP 150M] | 1fps - 60fps
| [420LongGOP 100M] |
| [422LongGOP 150M] | 1fps - 30fps
| [422ALL-I 400M]
| [3840×2160] | [HEVC LongGOP 150M] | 1fps - 60fps
| [420LongGOP 100M] |
| [422LongGOP 150M] | 1fps - 30fps
| [422ALL-I 400M]
| [2048×1080] | [422LongGOP 50M] | 1fps - 60fps
| [422ALL-I 100M]
| [1920×1080] | [422LongGOP 50M]
| [422ALL-I 100M]
| [AVCHD PH] | —
[S35 MIX 2.8K] | [2048×1080] | [422LongGOP 50M] | 1fps - 120fps
[422ALL-I 100M]
[1920×1080] | [422LongGOP 50M]
[422ALL-I 100M]
[4/3 CROP&MIX 2.2K] | [2048×1080] | [420LongGOP 50M] | 1fps - 240fps
[1920×1080] | [420LongGOP 50M]

## When [FREQUENCY] is set to [24.00p]

Can be set only when [SDI RAW] is set to [OFF].

[SENSOR MODE] | [MAIN PIXEL] | [MAIN CODEC] | VFR
--- | --- | --- | ---
[S35 5.7K] | [4096×2160] | [HEVC LongGOP 150M] | 1fps - 60fps
[420LongGOP 100M] |
[422LongGOP 150M] | 1fps - 30fps
[422ALL-I 400M]
[2048×1080] | [422LongGOP 50M] | 1fps - 60fps
[422ALL-I 100M]
[S35 MIX 2.8K] | [2048×1080] | [422LongGOP 50M] | 1fps - 120fps
[422ALL-I 100M]
[4/3 CROP&MIX 2.2K] | [2048×1080] | [420LongGOP 50M] | 1fps - 240fps

## When [FREQUENCY] is set to [25.00p]

Can be set only when [SDI RAW] is set to [OFF].

[SENSOR MODE] | [MAIN PIXEL] | [MAIN CODEC] | VFR
--- | --- | --- | ---
[S35 5.7K] | [4096×2160] | [HEVC LongGOP 150M] | 1fps - 50fps
| [420LongGOP 100M] |
| [422LongGOP 150M] | 1fps - 25fps
|  | [422ALL-I 400M] |
| [3840×2160] | [HEVC LongGOP 150M] | 1fps - 50fps
| [420LongGOP 100M] |
| [422LongGOP 150M] | 1fps - 25fps
|  | [422ALL-I 400M] |
| [2048×1080] | [422LongGOP 50M] | 1fps - 50fps
|  | [422ALL-I 100M] |
| [1920×1080] | [422LongGOP 50M] |
|  | [422ALL-I 100M] |
[S35 MIX 2.8K] | [2048×1080] | [422LongGOP 50M] | 1fps - 100fps
| [422ALL-I 100M] |
[1920×1080] | [422LongGOP 50M] |
|  | [422ALL-I 100M] |
[4/3 CROP&MIX 2.2K] | [2048×1080] | [420LongGOP 50M] | 1fps - 200fps
[1920×1080] | [420LongGOP 50M]

## When [FREQUENCY] is set to [29.97p]

Can be set only when [SDI RAW] is set to [OFF].

[SENSOR MODE] | [MAIN PIXEL] | [MAIN CODEC] | VFR
--- | --- | --- | ---
[S35 5.7K] | [4096×2160] | [HEVC LongGOP 150M] | 1fps - 60fps
| [420LongGOP 100M] |
| [422LongGOP 150M] | 1fps - 30fps
|  | [422ALL-I 400M] |
| [3840×2160] | [HEVC LongGOP 150M] | 1fps - 60fps
| [420LongGOP 100M] |
| [422LongGOP 150M] | 1fps - 30fps
|  | [422ALL-I 400M] |
| [2048×1080] | [422LongGOP 50M] | 1fps - 60fps
|  | [422ALL-I 100M] |
| [1920×1080] | [422LongGOP 50M] |
|  | [422ALL-I 100M] |
[S35 MIX 2.8K] | [2048×1080] | [422LongGOP 50M] | 1fps - 120fps
| [422ALL-I 100M] |
[1920×1080] | [422LongGOP 50M] |
|  | [422ALL-I 100M] |
[4/3 CROP&MIX 2.2K] | [2048×1080] | [420LongGOP 50M] | 1fps - 240fps
[1920×1080] | [420LongGOP 50M]

## When [FREQUENCY] is set to [50.00p]

Can be set only when [SDI RAW] is set to [OFF].

[SENSOR MODE] | [MAIN PIXEL] | [MAIN CODEC] | VFR
--- | --- | --- | ---
[S35 5.7K] | [4096×2160] | [HEVC LongGOP 200M] | 1fps - 50fps
|  | [420LongGOP 150M]
| [3840×2160] | [HEVC LongGOP 200M]
|  | [420LongGOP 150M] |
| [2048×1080] | [422LongGOP 100M] | 1fps - 50fps
|  | [422ALL-I 200M] |
| [1920×1080] | [422LongGOP 100M] |
| [422ALL-I 200M] |
| [AVCHD PS] | —
| [1280×720] | [AVCHD PM] | —
[S35 MIX 2.8K] | [2048×1080] | [422LongGOP 100M] | 1fps - 100fps
| [422ALL-I 200M] |
[1920×1080] | [422LongGOP 100M] |
|  | [422ALL-I 200M] |
[4/3 CROP&MIX 2.2K] | [2048×1080] | [420LongGOP 100M] | 1fps - 200fps
[1920×1080] | [420LongGOP 100M]

## When [FREQUENCY] is set to [59.94p]

Can be set only when [SDI RAW] is set to [OFF].

[SENSOR MODE] | [MAIN PIXEL] | [MAIN CODEC] | VFR
--- | --- | --- | ---
[S35 5.7K] | [4096×2160] | [HEVC LongGOP 200M] | 1fps - 60fps
|  | [420LongGOP 150M]
| [3840×2160] | [HEVC LongGOP 200M]
|  | [420LongGOP 150M] |
| [2048×1080] | [422LongGOP 100M] | 1fps - 60fps
|  | [422ALL-I 200M] |
| [1920×1080] | [422LongGOP 100M] |
| [422ALL-I 200M] |
| [AVCHD PS] | —
| [1280×720] | [AVCHD PM] | —
[S35 MIX 2.8K] | [2048×1080] | [422LongGOP 100M] | 1fps - 120fps
| [422ALL-I 200M] |
[1920×1080] | [422LongGOP 100M] |
|  | [422ALL-I 200M] |
[4/3 CROP&MIX 2.2K] | [2048×1080] | [420LongGOP 100M] | 1fps - 240fps
[1920×1080] | [420LongGOP 100M]

## When [FREQUENCY] is set to [59.94i]

Can be set only when [SDI RAW] is set to [OFF].

[SENSOR MODE] | [MAIN PIXEL] | [MAIN CODEC] | VFR
--- | --- | --- | ---
[S35 5.7K] | [1920×1080] | [422LongGOP 50M] | —
[422ALL-I 100M]
[AVCHD PH]
[AVCHD HA]

## When [FREQUENCY] is set to [50.00i]

Can be set only when [SDI RAW] is set to [OFF].

[SENSOR MODE] | [MAIN PIXEL] | [MAIN CODEC] | VFR
--- | --- | --- | ---
[S35 5.7K] | [1920×1080] | [422LongGOP 50M] | —
[422ALL-I 100M]
[AVCHD PH]
[AVCHD HA]

Top of the page