- Top
- Shooting
- Audio input
- When using an audio device or an external microphone

# When using an audio device or an external microphone

Connect an audio device or an external microphone to the <AUDIO INPUT 1>/<AUDIO INPUT 2> terminal.

Set each item in the [AUDIO SETTINGS] menu → [AUDIO INPUT].

Connected device | [AUDIO INPUT]
--- | ---
[INPUT1 LINE/MIC SEL]/[INPUT2 LINE/MIC SEL] | [INPUT1 MIC POWER]/[INPUT2 MIC POWER] | [INPUT1 MIC LEVEL]/[INPUT2 MIC LEVEL]*1 | [INPUT1 LINE LEVEL]/[INPUT2 LINE LEVEL]*2
Audio device | [LINE] | Disabled | Disabled | [4dB], [0dB]
External microphone | [MIC] | [OFF] | [−40dB], [−50dB], [−60dB] | Disabled
External microphone (with power supply) | [MIC] | [ON] | [−40dB], [−50dB], [−60dB] | Disabled

Factory setting: [−60dB]

Factory setting: [4dB]

NOTE

- When using a super-directional microphone AG-MC200G (optional), set [INPUT1 MIC LEVEL]/[INPUT2 MIC LEVEL] to [−50dB].

Top of the page