- Top
- Playback
- Thumbnail operation
- Playing back clips

# Playing back clips

From the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [FREQUENCY]/[MAIN PIXEL], select the system frequency and the number of recording pixels to play back.

From the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [MAIN CODEC], select the codec (MOV or AVCHD) to play back.

Press the <THUMBNAIL> button.

The thumbnail screen is displayed.

Press the <MENU> button while the thumbnail screen is displayed.

The menu is displayed.

From the [THUMBNAIL] menu → [PLAYBACK] → [SLOT SEL], select the card slot of the SD card to play back.

[ALL SLOT]: Displays the clips recorded on all the SD cards in each card slot. Displays in the order of the clips in card slot 1, and then clips in the card slot 2.

[SLOT1]: Displays only the clips recorded on the SD card in card slot 1.

[SLOT2]: Displays only the clips recorded on the SD card in card slot 2.

Select the clip to play back. (Fig. 1)

- is displayed on the clip that cannot be played back.

- To play back the clip with displayed, check the information of the clip with the clip information, and try operating from the beginning again.

## Playback from the operation icon

Direct playback bar

Playback operation | Operating procedure
--- | ---
Playback/pause | Touch /.
Fast-reverse playback | Touch . Speed will increase by touching twice.
Fast-forward playback | Touch . Speed will increase by touching twice.
Stop (return to thumbnail screen) | Touch .
Skip playback (cue up of the clip) | Touch the LCD monitor while playing back, and slide from right to left (left to right).
Slow playback | Touch and hold during pause. ( is for reverse slow playback) It will perform slow playback with continuous frame-by-frame while touched. It will return to normal speed playback by touching /. The frame-by-frame interval and the display time for each frame for the reverse slow playback differ depending on the type of the clip.
Frame-by-frame playback | Touch while paused. ( is reverse frame-by-frame playback) It will return to normal speed playback by touching /. The frame-by-frame interval for reverse frame-by-frame playback differs depending on the type of the clip.
Direct playback | Touch the direct playback bar, or slide it while touching. The playback video is paused during the operation. Playback is started by releasing the finger.

NOTE

- Operation of the camera or some of the operation may become slow for the clip with large file size.

- Operation of the camera or some of the operation may become slow when the there are large number of clips in the SD card.

- Playback will be paused when the [THUMBNAIL] menu → [PLAYBACK] → [SLOT SEL] → [ALL SLOT] is set and all clips in the SD cards are displayed. Playback is not possible across two SD cards.

- Playback will stop when the SD card is taken out while playing back.

Top of the page