- Top
- Preparation
- Mounting accessories
- Grip

# Grip

The grip is already mounted to the camera.

## Mounting the grip

Mount reference points

Fig. 1

Fig. 2

Grip cable clamp

<REMOTE> terminal

Grip cable

Fig. 3

Insert the grip to the camera. (Fig. 1)

- Align the mount reference points on the grip mounting section of the camera and the grip mounting section of the grip when inserting into the camera.

Slowly turn the grip counter-clockwise until it clicks. (Fig. 2)

Connect the grip cable to the <REMOTE> terminal. (Fig. 3)

Fix the grip cable with the grip cable clamp. (Fig. 3)

NOTE

- If it does not mount correctly, perform the mounting from the beginning. Do not apply excessive force to the grip and the camera.

- Store the grip cable inside the grip cable clamp. If it is not stored, the cable may fly out to bottom when the angle of grip is changed, or it may get caught when mounting a tripod.

- Try not to hold the whole camera only with the grip with the total mass of the whole camera has increased by attaching multiple accessories to the camera main body. The grip may get damaged.

#### Adjusting the angle of the grip

Grip rotation lever

Pull the grip rotation lever to the <UNLOCK> side.

Adjust the angle of the grip, and return the grip rotation lever at the position to fix.

The grip is fixed.

- The grip can be fixed in 8 different positions.

#### Adjusting the grip belt

The grip belt is already mounted to the grip.

Cover

Belt

Open the cover and adjust the length of the belt.

Replace the cover.

## Removing the grip

<GRIP RELEASE> button

Remove the grip cable from the grip cable clamp.

Remove the grip cable from the <REMOTE> terminal.

While pressing the <GRIP RELEASE> button on the camera, turn the grip clockwise.

NOTE

- Remove the grip after placing the camera body on a level location, such as desk.

Top of the page