- Top
- Specification
- Specifications
- Camera unit

# Camera unit

Pickup device | Super 35 mm, MOS sensor
Number of pixels | Total pixels: Approx. 20.49 million pixels (6340 (H) × 3232 (V)) Valid pixels: Approx. 17.52 million pixels (5720 (H) × 3016 (V))
Lens mount | EF mount
Optical filter | Built-in ND filter, electrical [ND:1.8]/[ND:1.2]/[ND:0.6]/[ND:CLR]
IR cut filter [ON]/[OFF] by assigning [IR SHOOTING] to the USER button (switched by menu)
Color temperature setting | ATW, AWB A, AWB B, 2000 K - 15000 K, −10.0GMg - +10.0GMg Up to 13 items can be registered
Gain setting | [ISO] mode Dual native ISO compatible, [200 ISO] to [25600 ISO] [dB] mode [NORMAL]/[HIGH] gain compatible, −12 dB to 26 dB (2 dB steps)
Shutter speed | When set to [deg] 3.0 deg - 357.0 deg (0.5 deg steps) Maximum of 12 items can be registered When set to [sec] 1/24.1 seconds to 1/8000 seconds (for 23.98p) Maximum of 12 items can be registered

Top of the page