- Top
- Output and Screen Display
- Output format
- Format that can be output from the <SDI OUT> terminal

# Format that can be output from the <SDI OUT> terminal

The format that can be output from the <SDI OUT> terminal differs with following combination of the settings.

- The [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [FREQUENCY]

- The [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [MAIN PIXEL]

- The [OUTPUT SETTINGS] menu → [SDI OUT] → [SIGNAL SEL]

- The [OUTPUT SETTINGS] menu → [SDI OUT] → [OUT FORMAT]

Item | Output Format [OUT FORMAT]
--- | ---
[FREQUENCY] | [MAIN PIXEL] | [SIGNAL SEL]
[59.94p] [50.00p] | [4096×2160] | [SDI] | (No 4K output) 1920×1080p*1 1920×1080i*1 (Factory settings)
|  | [LCD(1080p)] | 1920×1080p*2
|  | [LCD(1080i)] | 1920×1080i*2
| [3840×2160] | [SDI] | (No 4K output) 1920×1080p 1920×1080i(Factory settings)
|  | [LCD(1080p)] | 1920×1080p*2
|  | [LCD(1080i)] | 1920×1080i*2
| [2048×1080] | [SDI] | 1920×1080p*1 1920×1080i*1 (Factory setting)
|  | [LCD(1080p)] | 1920×1080p*2
|  | [LCD(1080i)] | 1920×1080i*2
| [1920×1080] | [SDI] | 1920×1080p 1920×1080i (Factory setting)
|  | [LCD(1080p)] | 1920×1080p*2
|  | [LCD(1080i)] | 1920×1080i*2
| [1280×720] | [SDI] | 1280×720p (Factory setting)
|  | [LCD(1080p)] | 1920×1080p*2
|  | [LCD(1080i)] | 1920×1080i*2
[59.94i] [50.00i] | [1920×1080] | [SDI] | 1920×1080i (Factory setting)
|  | [LCD(1080p)] | 1920×1080p*2
|  | [LCD(1080i)] | 1920×1080i*2
[29.97p] [23.98p] | [4096×2160] | [SDI] | 4096×2160p 1920×1080p*1 1920×1080PsF*1 (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 59.94p*2
|  | [LCD(1080i)] | 1920×1080 over 59.94i*2
| [3840×2160] | [SDI] | 3840×2160p 1920×1080p 1920×1080PsF (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 59.94p*2
|  | [LCD(1080i)] | 1920×1080 over 59.94i*2
| [2048×1080] | [SDI] | 1920×1080p*1 1920×1080PsF*1 (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 59.94p*2
|  | [LCD(1080i)] | 1920×1080 over 59.94i*2
| [1920×1080] | [SDI] | 1920×1080p 1920×1080PsF (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 59.94p*2
|  | [LCD(1080i)] | 1920×1080 over 59.94i*2
[24.00p] | [4096×2160] | [SDI] | 4096×2160p 1920×1080p*1 1920×1080PsF*1 (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 60p*2
|  | [LCD(1080i)] | 1920×1080 over 60i*2
| [2048×1080] | [SDI] | 1920×1080p*1 1920×1080PsF*1 (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 60p*2
|  | [LCD(1080i)] | 1920×1080 over 60i*2
[25.00p] | [4096×2160] | [SDI] | 4096×2160p 1920×1080p*1 1920×1080PsF*1 (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 50p*2
|  | [LCD(1080i)] | 1920×1080 over 50i*2
| [3840×2160] | [SDI] | 3840×2160p 1920×1080p 1920×1080PsF (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 50p*2
|  | [LCD(1080i)] | 1920×1080 over 50i*2
| [2048×1080] | [SDI] | 1920×1080p*1 1920×1080PsF*1 (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 50p*2
|  | [LCD(1080i)] | 1920×1080 over 50i*2
| [1920×1080] | [SDI] | 1920×1080p 1920×1080PsF (Factory setting)
|  | [LCD(1080p)] | 1920×1080 over 50p*2
|  | [LCD(1080i)] | 1920×1080 over 50i*2

Displayed in the letterbox format. Quality is slightly lower compared to recorded image.

It will be the same image as the LCD monitor with black band in all four sides. Focus and EI assist display are possible. Equivalent to 4:2:2 (8 bits).

NOTE

- The output will be as follows regardless of [FREQUENCY] or [MAIN PIXEL] setting when [SIGNAL SEL] is set to [LCD(1080p)] or [LCD(1080i)].

  - When [FREQUENCY] is set to [59.94p]/[59.94i]/[29.97p]/[23.98p]: 1920×1080 over 59.94p or 1920×1080 over 59.94i

  - When [FREQUENCY] is set to [50.00p]/[50.00i]/[25.00p]: 1920×1080 over 50p or 1920×1080 over 50i

  - When [FREQUENCY] is set to [24.00p]: 1920×1080 over 60p or 1920×1080 over 60i

- The 2048×1080 output is not supported.

- [OUT FORMAT] will change to the factory setting when settings of [FREQUENCY] and [MAIN PIXEL] change and current settings in [OUT FORMAT] cannot be acquired.

- The output format when playing back from the thumbnail screen is as follows.

  - It will be the value set in [OUT FORMAT] when the recording resolution of the playback clip is the same as [MAIN PIXEL].

  - It will be factory setting of [OUT FORMAT] when the recording resolution of the playback clip is different from [MAIN PIXEL].

- When the [SYSTEM SETTINGS] menu → [SYSTEM MODE] → [SDI RAW] is set to anything other than [OFF], it will be RAW output.

Top of the page