- Top
- Preparation
- Assigning function to the USER buttons
- Functions assigned to USER buttons

# Functions assigned to USER buttons

## Function assigned to <USER 1> to <USER 9> buttons

Item | Description
--- | ---
[INHIBIT] | Disables assignment of functions.
[AWB] | Enables/disables the auto white balance.
[ONE PUSH AF] | Assigns the one-push auto focus function.
[ONE PUSH A.IRIS] | Assigns the one-push auto iris function.
[ATW LOCK] | Fixes the value of the white balance. Pressing the USER button again will resume the operation of the auto tracking white balance. Enable when the auto tracking white balance is operating.
[E.I.S.] | Enables/disables the electronic image stabilization function.
[D.ZOOM] | Enables/disables the digital zoom. It will zoom the angle of view 1.4 times both vertically and horizontally.
[IR SHOOTING] | Enables/disables the IR recording.
[REC SW] | Starts or stops the recording.
[PRE REC] | Enables/disables the pre-recording.
[VFR] | Enables/disables the variable frame rate recording function.
[REC CHECK] | Automatically plays back the last approximately three seconds of the previously shot clip.
[DEL LAST CLIP] | Deletes the clip last shot.
[SLOT SEL] | Selects the card slot with the SD card to record inserted. Or, switches the card slot for the clip to display in the thumbnail screen.
[EXPAND] | Enables/disables the enlarged display function (focus assist function).
[OPEN IRIS F.A.] | Assigns the open iris focus assist function (focus assist function).
[PEAK./SQUARES F.A.] | Enables/disables the peaking function and focus square display (focus assist function). The display is selected in the [OUTPUT SETTINGS] menu → [LCD FOCUS ASSIST] → [PEAK./SQUARES MODE].
[WFM] | Switches the display of the waveform monitor. The waveform display is selected in the [OUTPUT SETTINGS] menu → [LCD EI ASSIST] → [WFM MODE].
[SPOT METER] | Displays/hides the spot meter. This is enabled when the [OUTPUT SETTINGS] menu → [SDI/HDMI INDICATOR]/[LCD INDICATOR] → [SPOT METER] → [ON] is set.
[ZEBRA] | Displays/hides zebra patterns.
[LEVEL GAUGE] | Displays/hides the level gauge.
[LEVEL GAUGE SET] | Sets the current horizontal and vertical direction as the reference value of the level gauge.
[SDI COLOR] | Switches the output image from the <SDI OUT> terminal.
[HDMI COLOR] | Switches the output image from the <HDMI> terminal.
[LCD COLOR] | Switches the output image from the <LCD> terminal.
[SDI OUT HDR] | Switches the high dynamic range/standard dynamic range for the output image from the <SDI OUT> terminal.
[HDMI OUT HDR] | Switches the high dynamic range/standard dynamic range for the output image from the <HDMI> terminal.
[LCD HDR] | Switches the high dynamic range/standard dynamic range for the output image from the <LCD> terminal.
[LCD CLEAN VIEW] | Erases the display of the indicator or marker superimposed to the output video from the <LCD> terminal.
[LCD MARKER] | Displays/hides the marker superimposed in the output video from the <LCD> terminal.
[COLOR BARS] | Displays/hides the color bars.
[LOAD SETUP FILE] | Selects the setup file saved in the SD card and reads it into the camera.
[POWER LCD] | Make it easier to view the LCD monitor in a well-lighted area such as outdoor.

NOTE

- Following functions will be disabled when the camera is set to < > (standby) and then turned on again.

  [ATW LOCK], [D.ZOOM], [EXPAND], [PEAK./SQUARES F.A.], [WFM], [SPOT METER], [LCD CLEAN VIEW], [COLOR BARS], [POWER LCD]

- Following functions will be enabled when the camera is set to < > (standby) and then turned on again.

  [LCD MARKER]

## Functions assigned to the multidial

When <WB>/<USER>/<ISO/dB> switch is set to <USER>, the multidial can be used as a USER button.

- The operation as the USER button is enabled when the VIEW screen is displayed.

Item | Description
--- | ---
[INHIBIT] | Disables assignment of functions.
[SHUTTER] | Enables/disables the shutter function when the multidial is pressed. The setting value of the shutter speed can be selected by turning the multidial.
[FPS] | Enables/disables the variable frame rate record function when the multidial is pressed. The setting value of the frame rate can be selected by turning the multidial.
[MONITOR VOL] | The adjustment of the audio level output from the headphones terminal is enabled when the multidial is pressed. The level meter for adjusting is displayed in the LCD monitor when it is enabled. The level of the audio can be adjusted by turning the multidial. Level adjustment of audio is ended by pressing the multidial again.

Top of the page