- Top
- Preparation
- Tally lamp

# Tally lamp

The front tally lamp and the rear tally lamp can be illuminated during the shooting.

Select the [SYSTEM SETTINGS] menu → [LED & FAN] → [TALLY LED] → [FRONT]/[REAR]/[BOTH].

- The tally lamp will flash when the camera is in the following status.

  - When the remaining capacity of the SD card or the remaining battery level is low (one time per second)

  - The SD card has no more space to record (four times per second)

  - When a warning such as a system error or a recording abnormality has occurred (four times per second)

NOTE

- The tally lamp will not illuminate or flash when the [SYSTEM SETTINGS] menu → [LED & FAN] → [TALLY LED] → [OFF] is set.

Top of the page