- Top
- Description of Parts
- Camera
- Rear side

# Rear side

Following terminals, card slots, and card access lamps are inside the cover.

- <HDMI> terminal

- <USB2.0 HOST> terminal

- <SERVICE> terminal

- Headphone terminal

- <SDI OUT> terminal

- <TC IN/OUT> terminal

- <DC IN 12V> terminal

- Card slot 1/card slot 2

- Card 1 access lamp/card 2 access lamp

1. Card 1 access lamp

   Indicates the access status for recording and playback of the SD card inserted in the card slot 1.

   To flash the lamp or not can be set in the menu.

2. Card slot 1

   Slot for SD card.

3. Card slot 2

   Slot for SD card.

4. Card 2 access lamp

   Indicates the access status for recording and playback of the SD card inserted in the card slot 2.

   To flash the lamp or not can be set in the menu.

5. <SLOT SEL>/<USER 7> button

   Selects the card slot to record to or playback from.

   Also, this is also used as the USER button (USER7).

6. Rear tally lamp

   Illuminates when the recording is started. Flashes when the battery level becomes low.

   To flash the lamp or not can be set in the menu.

7. <AUDIO INPUT 1>/<AUDIO INPUT 2> terminal (XLR, 3-pin)

   Connects an audio equipment or an external microphone.

8. <HDMI> terminal

   A terminal to output video signal by connecting a monitor, etc.

9. <USB2.0 HOST> terminal

   Can connect to wireless LAN when the wireless module (optional) compatible to camera is mounted.

10. <SERVICE> terminal

    A maintenance terminal.

11. Battery release button

    Used when removing the battery from the camera.

12. Headphone terminal

    Connects audio monitoring headphones.

13. <SDI OUT> terminal

    A terminal to output SDI signal by connecting a monitor, etc.

14. Fan outlet

    Fan outlet for cooling fan. Do not block this while the camera is being used.

15. Battery mounting section

    Mounts a battery.

16. <DC IN 12V> terminal

    Connects the supplied AC adaptor and supplies an external power supply.

17. <TC IN/OUT> terminal

    Connects to an external equipment and output/input a time code.

    Inputs the standard time code when locking the time code with an external equipment.

    Input and output are set in the [REC SETTINGS] menu → [TC] → [TC IN/OUT SEL].

Top of the page