- Top
- Shooting
- Convenient shooting functions
- Zebra patterns display

# Zebra patterns display

The camera can display two types of zebra patterns to the output image from the <LCD> terminal.

Select the [OUTPUT SETTINGS] menu → [LCD EI ASSIST] → [ZEBRA] → [ON].

- Factory setting: [OFF]

## Setting the detection level

Set the [OUTPUT SETTINGS] menu → [LCD EI ASSIST] → each item.

Item | Description of settings
--- | ---
[ZEBRA1 DETECT] | Sets the detection level of zebra pattern 1. [0%]…[109%] (Factory setting: [80%])
[ZEBRA2 DETECT] | Sets the detection level of zebra pattern 2. [0%]…[109%] (Factory setting: [100%])
[ZEBRA2] | Enables/disables zebra pattern 2 and selects [SPOT]. [ON], [SPOT], [OFF] (Factory setting: [OFF])

#### Display area of the zebra pattern

The display area of the zebra pattern varies depending on the [OUTPUT SETTINGS] menu → [LCD EI ASSIST] setting.

When [SPOT] is selected in [ZEBRA2], the area corresponding to the [ZEBRA1 DETECT] setting value to the [ZEBRA2 DETECT] setting value is displayed in zebra pattern.

[ZEBRA2]

[ON]

[OFF]

[SPOT]

[109%]

[ZEBRA2 DETECT]

[ZEBRA1 DETECT]

[0%]

NOTE

- The zebra pattern cannot be recorded.

- When the focus square display of the focus assist function is enabled, the zebra pattern is not displayed while displaying the color bars.

Top of the page