- Top
- Shooting
- Audio input
- Direct volume control function

# Direct volume control function

The audio level can be adjusted with the multidial by assigning [MONITOR VOL] to the multidial that is to be used as the USER button in advance.

- To use as the USER button, set the <WB>/<USER>/<ISO/dB> switch to <USER>.

#### Assigning [MONITOR VOL] to the multidial

Select the [SYSTEM SETTINGS] menu → [USER SWITCHES] → [USER TOGGLE] → [MONITOR VOL].

#### Using the direct volume control function

Set the <WB>/<USER>/<ISO/dB> switch to <USER>.

Operate the multidial to adjust the audio level.

Top of the page