- Top
- Connecting to External Devices
- Connecting the camera and the iPad/Android terminal
- Connecting to the wireless access point ([INFRA(SELECT)]/[INFRA(MANUAL)])

# Connecting to the wireless access point ([INFRA(SELECT)]/[INFRA(MANUAL)])

This is the setting to connect the camera to a wireless access point.

## When connecting by searching the wireless access point (SSID)

Select the [NETWORK SETTINGS] menu → [NETWORK PROPERTY] → [TYPE] → [INFRA(SELECT)].

From the [NETWORK SETTINGS] menu → [NETWORK PROPERTY], set each item as necessary.

- For details of setting, refer to “Setting items in [NETWORK PROPERTY] when set to [INFRA(SELECT)]”.

Select the [NETWORK SETTINGS] menu → [NETWORK SEL] → [WLAN].

Select the [NETWORK SETTINGS] menu → [NETWORK PROPERTY] → [SSID].

- Displays SSID of the searched wireless access point.

Select SSID, and select [Enter].

Setting is completed when the [ENCRYPT KEY] (encryption key, password) is not set.

If the [ENCRYPT KEY] is set, enter the password, and select [Enter].

Check the network connection.

Once connected, is displayed on the screen of the camera.

NOTE

- ENCRYPTION in WEP is not supported.

#### Setting items in [NETWORK PROPERTY] when set to [INFRA(SELECT)]

[ENCRYPTION] | [WPA-TKIP], [WPA-AES], [WPA2-TKIP], [WPA2-AES], [NONE] (Factory setting: [WPA-AES])
[ENCRYPT KEY] | WPA2 encryption key (Factory setting: [01234567890123456789abcdef])
[DHCP] | Setting the DHCP function [OFF]: Does not use the DHCP function. [CLIENT]: Acquire from DHCP when connecting with [TYPE] set to [INFRA(SELECT)] or [INFRA(MANUAL)]. [SERVER]: When connecting by setting [TYPE] to [DIRECT], enable the DHCP server function of the camera. (Cannot be selected.) (Factory setting: [SERVER])
[IP ADDRESS] | IP address of the camera (Factory setting: [192.168.0.1])
[SUBNET MASK] | Subnet mask (Factory setting: [255.255.255.0])

## When entering the wireless access point (SSID) manually

Select the [NETWORK SETTINGS] menu → [NETWORK PROPERTY] → [TYPE] → [INFRA(MANUAL)].

Set each item in the [NETWORK SETTINGS] menu → [NETWORK PROPERTY] as necessary.

- For details of setting, refer to “Setting items in [NETWORK PROPERTY] when set to [INFRA(MANUAL)]”.

Select the [NETWORK SETTINGS] menu → [NETWORK SEL] → [WLAN].

From the [NETWORK SETTINGS] menu → [NETWORK PROPERTY] → [SSID], enter the SSID of the wireless access point to connect.

Select SSID, and select [Enter].

Setting is completed when the [ENCRYPT KEY] (encryption key, password) is not set.

If the [ENCRYPT KEY] is set, enter the password, and select [Enter].

Check the network connection.

Once connected, is displayed on the screen of the camera.

NOTE

- ENCRYPTION in WEP is not supported.

#### Setting items in [NETWORK PROPERTY] when set to [INFRA(MANUAL)]

[ENCRYPTION] | [WPA-TKIP], [WPA-AES], [WPA2-TKIP], [WPA2-AES], [NONE] (Factory setting: [WPA-AES])
[ENCRYPT KEY] | WPA2 encryption key (Factory setting: [01234567890123456789abcdef])
[DHCP] | Setting the DHCP function [OFF]: Does not use the DHCP function. [CLIENT]: Acquire from DHCP when connecting with [TYPE] set to [INFRA(SELECT)] or [INFRA(MANUAL)]. [SERVER]: When connecting by setting [TYPE] to [DIRECT], enable the DHCP server function of the camera. (Cannot be selected.) (Factory setting: [SERVER])
[IP ADDRESS] | IP address of the camera (Factory setting: [192.168.0.1])
[SUBNET MASK] | Subnet mask (Factory setting: [255.255.255.0])

## When connecting from the history

History of connection is saved when connected to a wireless access point. Connection is easily made with the same setting as before when connecting from the history.

Select the [NETWORK SETTINGS] menu → [CONNECTION HISTORY] → [SELECT].

The connection history is listed with the SSID of the wireless access point.

Select the SSID to connect.

Check the network connection.

Once connected, is displayed on the screen of the camera.

## When deleting the history

Select the [NETWORK SETTINGS] menu → [CONNECTION HISTORY] → [DELETE].

The connection history is listed with the SSID of the wireless access point.

Select the SSID to delete.

A confirmation message appears.

Select [SET].

Returns to Step 2.

- To not to delete, select .

To continue to delete, perform Steps 2 to 3.

To exit from the operation, select the [EXIT] button.

NOTE

- Maximum of 20 histories that were recently used can be saved.

Top of the page