- Top
- Preparation
- Assembling modules
- Mounting the Electronic HD color viewfinder

# Mounting the Electronic HD color viewfinder

Lock

Release

Fig. 1

Fig. 2

Attach the slider unit to the viewfinder mounting holes on top of the camera module using the two supplied screws. (Fig. 1)

Slide the viewfinder plate from above into the slider unit. (Fig. 2)

Release the viewfinder lock lever by pushing it forward.

Push down the lock lever backwards to lock.

Connect the supplied connecting cable to the viewfinder connection terminal and the camera module’s <VF> terminal.

Connect by aligning the red mark on the connector.

## Disassembling

1. Stopper

Remove the connecting cable.

Push down the lock lever towards the front to release the lock.

Lift the viewfinder while pulling the stopper.

Remove the slider unit clamping screw.

Top of the page