- Top
- Control Panel
- Control panel operation
- Camera status display

# Camera status display

1. Recording status display

   Top: Main slot recording status display

   - [REC]: Currently recording

     : When audio is not being recorded

   Bottom: Sub slot recording status display

   - [REC]: Currently recording

2. Media free space display

   Top: Main slot media remaining capacity display

   Bottom: Sub slot media remaining capacity display

   - [min]: Remaining capacity (0 to 599 minutes)

   - [h]: Remaining capacity (more than 10 hours)

   - [END]: No remaining free space

   - [WP]: Write protected

   - [OFF]: When [SUB CODEC] is [OFF]

3. Codec display

   Top: Main slot codec display ([MAIN CODEC] setting value)

   Bottom: Sub slot codec display ([SUB CODEC] setting value)

4. Battery display

   - Changes to → → → as the battery charge level gets lower.

   - (yellow): Battery charge level is low.

   - (red): Battery charge has run out.

   - [.V]: Displays the battery charge level in units of 0.1 V.

   - [%]: Displays the battery charge level with charge level information in %.

5. Audio level meter display

   - Channel display

     [1]/[2] or [3]/[4]

   - Level meter display

     Displays the level represented by 19 bars. (2 dB increments)

   - Standard level bar

     At the −18 dB position or the −20 dB position

     The standard is in [MENU] → [SYSTEM SETTINGS] → [AUDIO LEVEL] → [HEADROOM]

6. Warning/error displays

   : Warning (details are displayed on the time code display in the following cases)

   - [SYSTEM ERROR !]

   - [TURN POWER OFF !]

   - [REC WARING !]

   - [CARD ERROR !] (when recording has stopped)

   - [LOW BATTERY !]

   - [MEDIA END !]

   : Alert

7. Time code display

   - [TCG 12:59:59:20]: Displays the time code generator value.

   - [TCR 12:59:59:20]: Displays the time code reader value.

   - [UBG AB CD EF 98]: Displays the user bits generator value.

   - [UBR AB CD EF 98]: Indicates the user bits reader value.

   - [Dur.00:59:59:23]: Displays the duration.

8. [USER CLIP NAME]/[TYPE3] display

   Displays the CAM INDEX, REEL number, and clip number.

9. Lock display/network status display

   Displayed when button operations are disabled due to the <LOCK> switch.

   : Displays the network connection status.

Top of the page