- Top
- Other Useful Functions
- Setting the time data
- User bits settings

# User bits settings

Sets the user bits to be recorded in the sub code area with the control panel.

Item | Description
--- | ---
[USER] | Records internal user values. The user value can be set from [MENU] → [REC SETTINGS] → [TC] → [SET UB], the user value can be set. Setting values are held even when the power is turned off. For details, refer to “How to input user bits”.
[TIME] | Records the time measured by the internal clock.
[DATE] | Records the hour digit of year/month/day/date-time measured by the internal clock.
[EXT INPUT] | Records the user bits values currently entered to the <TC IN/OUT> terminal.
[TCG] | Records the time code value.
[FRAME RATE] | Records the camera photo frame rate information. When playing back clips recorded in native format, the same frame rate information as VITC UB is output regardless of the recorded value. Use at this setting when the editing device such as a computer uses the frame rate information of the user bits.

Top of the page