- Top
- Preparation
- Mounting and adjusting the lens
- Mounting the lens

# Mounting the lens

Lens lever

Mount cap

Fig. 1

Fig. 2

Cable clamp

<LENS> terminal

Fig. 4

Fig. 3

Raise the lens lever and remove the mount cap. (Fig. 1)

Align the convex portion at the upper right of the lens mount with the concave portion at the lens mount to mount the lens. (Fig. 2)

Lower the lens lever to firmly clamp the lens. (Fig. 3)

If a cable is attached to the lens, secure the cable through the cable clamp and connect it to the <LENS> terminal. (Fig. 4)

NOTE

- For handling the lens, refer to the lens operating instructions.

- When the lens is removed, install the mount cap to protect the device.

Top of the page