- Top
- Viewfinder
- Convenient shooting functions
- Zebra patterns display

# Zebra patterns display

The camera can display two types of zebra patterns.

The level to display the zebra pattern can be set in [MENU] → [OUTPUT SETTINGS] → [VF EI ASSIST] → [ZEBRA].

Item | Description of settings
--- | ---
[ZEBRA SW] | Sets whether to superimpose the zebra signal on the output from the <VF> terminal and <VF SDI> terminal. [ON], [OFF] Factory setting: [OFF]
[ZEBRA1 DETECT] | Sets the detection level of zebra pattern 1. [0%]…[109%] Factory setting: [80%]
[ZEBRA2 DETECT] | Sets the detection level of zebra pattern 2. [0%]…[109%] Factory setting: [100%]
[ZEBRA2 MODE] | Enables/disables zebra pattern 2 and selects [SPOT]. [ON], [SPOT], [OFF] Factory setting: [OFF]

[SPOT]: The image level from the setting value of [ZEBRA1 DETECT] to the setting value of [ZEBRA2 DETECT] is displayed in the zebra pattern.

[ZEBRA2]

Image level

[ON]

[OFF]

[SPOT]

[109%]

[ZEBRA2 DETECT]

[ZEBRA1 DETECT]

[0%]

Top of the page