- Top
- Description of Parts
- Camera module
- Front

# Front

1. Accessory mounting holes

   For attaching accessories.

   - Mounting hole size

     - 3/8-16 UNC (screw length 5.5 mm or shorter)

2. Lens cable /microphone cable clamp

   Clamp for securing the lens and microphone cables.

3. Lens mount

   Holds the lens.

4. <FILTER> dial

   Selects a filter which suits the illumination of the subject.

   <1><CLEAR>: Does not use the ND filter.

   <2><0.6ND>: Reduces the amount of light entering the MOS sensor to 1/4.

   <3><1.2ND>: Reduces the amount of light entering the MOS sensor to 1/16.

   <4><1.8ND>: Reduces the amount of light entering the MOS sensor to 1/64.

5. Lens lever

   After mounting the lens to the lens mount, tighten the lever to secure the lens.

6. Mount cap

   Attach the cap when the lens is not mounted.

Top of the page