- Top
- Menu Operations
- Menu list
- [OUTPUT SETTINGS]

# [OUTPUT SETTINGS]

Sets the display content of the output video from the viewfinder and <VF SDI> terminal.

Item | Description of settings
--- | ---
[SDI OUT] | [P to PsF] | Sets the segment frame for the output from terminals <SDI OUT1> to <SDI OUT4>. When [MENU] → [CAMERA SETTINGS] → [FPS] → [VFR SW] is set to [OFF] The setting is enabled when the following conditions are fulfilled. When [MENU] → [SYSTEM SETTINGS] → [MAIN PIXEL] is set to [2048×1080] or [1920×1080] When [MENU] → [SYSTEM SETTINGS] → [FREQUENCY] is set to [23.98p], [24.00p], [25.00p], or [23.98p] When [MENU] → [CAMERA SETTINGS] → [FPS] → [VFR SW] is set to [ON] The setting is enabled when the following conditions are fulfilled. When [MENU] → [SYSTEM SETTINGS] → [MAIN PIXEL] is set to [2048×1080] or [1920×1080] When [MENU] → [SYSTEM SETTINGS] → [FREQUENCY] is set to [23.98p], [24.00p], [25.00p], or [23.98p] When [MENU] → [SYSTEM SETTINGS] → [MAIN CODEC] is set to [ProRes 4444 XQ] or [ProRes 4444] [ON], [OFF] Factory setting: [OFF]
| [4K OUT TYPE] | Sets the 4K signal format to be output from terminals <SDI OUT1> to <SDI OUT4>. [SQUARE], [2 SAMPLE INT] Factory setting: [SQUARE]
| [3G-SDI OUT] | Sets the 3G SDI signal format to be output from terminals <SDI OUT1> to <SDI OUT4>. [LEVEL-A]: Selects the LEVEL-A method. [LEVEL-B]: Selects the LEVEL-B DL method. Factory setting: [LEVEL-B]
| [SDI REC REMOTE] | Sets whether to use the control function of recording operation for an external device (such as a recorder) connected to the <SDI OUT> terminal, the <MON OUT1> terminal, and the <MON OUT2> terminal. It can be output from the <MON OUT2> terminal only when [MON OUT2 SIGNAL SEL] is set to [MON OUT1]. [ON]: Controls the recording operation of the external device. [OFF]: Does not control the recording operation of the external device. Factory setting: [OFF]
[MON OUT] | [MON OUT FORMAT] | Select the signal output from the <MON OUT1> terminal and <MON OUT2> terminal. Selectable items vary depending on the settings of [MENU] → [SYSTEM SETTINGS] → [FREQUENCY] and [MENU] → [SYSTEM SETTINGS] → [MAIN CODEC]. When [FREQUENCY] is set to [23.98p]: [MAIN CODEC] is set to [AVC-Intra4K 444], [AVC-Intra2K 444], or [AVC-Intra444] [1920/23.98PsF] [MAIN CODEC] is set to anything other than [AVC-Intra4K 444], [AVC-Intra2K 444], or [AVC-Intra444] [1920/23.98PsF], [1920 over 59.94p], [1920 over 59.94i] When [FREQUENCY] is set to [24.00p]: [MAIN CODEC] is set to [AVC-Intra4K 444] or [AVC-Intra2K 444] [1920/24PsF] [MAIN CODEC] is set to anything other than [AVC-Intra4K 444] or [AVC-Intra2K 444] [1920/24PsF], [1920 over 60p], [1920 over 60i]
|  | When [FREQUENCY] is set to [25.00p]: [MAIN CODEC] is set to [AVC-Intra4K 444], [AVC-Intra2K 444], or [AVC-Intra444] [1920/25PsF] [MAIN CODEC] is set to anything other than [AVC-Intra4K 444], [AVC-Intra2K 444], or [AVC-Intra444] [1920/25PsF], [1920 over 50p] When [FREQUENCY] is set to [29.97p]: [MAIN CODEC] is set to [AVC-Intra4K 444], [AVC-Intra2K 444], or [AVC-Intra444] [1920/29.97PsF] [MAIN CODEC] is set to anything other than [AVC-Intra4K 444], [AVC-Intra2K 444], or [AVC-Intra444] [1920/29.97PsF], [1920 over 59.94p]
|  | When [FREQUENCY] is set to [50p]: [1920/50p], [1920/50i] When [FREQUENCY] is set to [50i]: [1920/50i] When [FREQUENCY] is set to [59.94p]: [1920/59.94p], [1920/59.94i] When [FREQUENCY] is set to [59.94i]: [1920/59.94i]
|  | Factory setting: [1920/23.98PsF]
| [3G-SDI OUT] | Sets the 3G SDI signal format to be output from the <MON OUT1> terminal and <MON OUT2> terminal. [LEVEL-A]: Selects the LEVEL-A method. [LEVEL-B]: Selects the LEVEL-B DL method. Factory setting: [LEVEL-B]
| [MON OUT2 SIGNAL SEL] | Sets the output from the <MON OUT2> terminal. [VF SDI (1080p)]: Selects the same output as the <VF SDI> terminal. The signal format will always be 1920×1080p. [VF SDI (1080i)]: Selects the same output as the <VF SDI> terminal. The signal format will always be 1920×1080i. [MON OUT1]: Selects the same output as the <MON OUT1> terminal. Factory setting: [VF (1080p)]
| [MON OUT1 STATUS] | Sets whether to show the status display on the output from the <MON OUT1> terminal. [ON], [OFF] Factory setting: [OFF]
| [MON OUT2 STATUS] | Sets whether to show the status display on the output from the <MON OUT2> terminal. [ON], [OFF] Factory setting: [OFF]
| [MENU DISP] | Sets whether to display [MENU] in the output from the <MON OUT1> terminal and <MON OUT2> terminal. [ON], [OFF] Factory setting: [ON]
| [PLAY DISP & CTRL] | Sets whether to display the PLAY screen in the output from the <MON OUT1> terminal and the <MON OUT2> terminal. [ON], [OFF] Factory setting: [OFF]
[VF OUT] | [VF SDI OUT FORMAT] | Selects the signal to output from the <VF SDI> terminal. [1080P], [1080i] Factory setting: [1080P]
| [PLAYBACK VF IMAGE] | Selects the image output from the <VF> terminal and the <VF SDI> terminal. [PLAYBACK], [CAMERA] Factory setting: [PLAYBACK]
| [SURROUND VIEW SW] | Enables/disables the surround view function (the function to display the image outside the effective range on the viewfinder). [ON], [OFF] Factory setting: [OFF]
| [SURROUND VIEW AREA] | Selects the range of the surround view. [UPPER (NORMAL)], [LOWER] The image to be recorded will shift approximately 396 µm upwards from the center of the lens when [LOWER] is selected. Take care when the zoom lens is used. Factory setting: [UPPER (NORMAL)]
| [SURROUND VIEW LINE SW] | Enables/disables the effective area line mark display function. [ON], [OFF] Factory setting: [ON]
| [SURROUND VIEW COLOR] | Sets the effective area line mark color. [WHITE], [BLACK], [RED], [GREEN], [BLUE], [YELLOW] Factory setting: [WHITE]
| [SURROUND VIEW LEVEL] | Sets the microphone level for the surround signal. [OFF], [75%], [50%], [25%] Factory setting: [OFF]
| [SMOOTH MODE] | Enables/disables the smooth mode (function which smoothens the viewfinder image when 24P and half shutter function is running). [ON], [OFF] Factory setting: [OFF]
[MON OUT INDICATOR] | [SYSTEM PIXEL] | Displays/hides system pixels. [ON], [OFF] Factory setting: [ON]
| [SYSTEM FREQ] | Displays/hides system frequency. [ON], [OFF] Factory setting: [ON]
| [REC FORMAT] | Displays/hides recording format display. [ON], [OFF] Factory setting: [ON]
| [REC MODE] | Displays/hides the status for the interval recording or the pre-recording. [ON], [OFF] Factory setting: [ON]
| [VFR] | Displays/hides the variable frame rate status. [ON], [OFF] Factory setting: [ON]
| [FPS] | Displays/hides frame rate. [ON], [OFF] Factory setting: [ON]
| [SHUTTER] | Displays/hides shutter speed. [ON], [OFF] Factory setting: [ON]
| [EI] | Displays/hides EXPOSURE INDEX. [ON], [OFF] Factory setting: [ON]
| [WHITE] | Displays/hides color temperature. [ON], [OFF] Factory setting: [ON]
| [IRIS] | Displays/hides iris value. [ON], [OFF] Factory setting: [ON]
| [FOCUS] | Displays/hides focus distance. [ON], [OFF] Factory setting: [ON]
| [ZOOM] | Displays/hides zoom value. [ON], [OFF] Factory setting: [ON]
| [FILTER] | Displays/hides the optical filter transmittance. [ON], [OFF] Factory setting: [ON]
| [EXTENDER] | Displays/hides the extender. [ON], [OFF] Factory setting: [ON]
| [Y GET] | Displays/hides brightness of Y GET. [ON], [OFF] Factory setting: [ON]
| [TC] | Displays/hides the time code, user bits, and duration counter displays. [TCG/TCR], [TCG], [OFF] Factory setting: [TCG/TCR]
| [P2 CARD REMAIN] | Displays/hides the display of the remaining recording free space of a P2 card. [ON], [OFF] Factory setting: [ON]
| [BATTERY REMAIN] | Displays/hides the estimated remaining battery charge level. [ON], [OFF] Factory setting: [ON]
| [PROXY] | Displays/hides proxy information. [ON], [OFF] Factory setting: [ON]
| [GPS] | Displays/hides GPS signal reception status. [ON], [OFF] Factory setting: [OFF]
| [CLIP NAME] | Displays/hides clip names. [ON], [OFF] Factory setting: [ON]
| [USER CLIP NAME (TYPE3)] | Displays/hides the user clip name when [REC SETTINGS] → [REC METADATA] → [USER CLIP NAME] is set to [TYPE3]. [ON], [OFF] Factory setting: [OFF]
| [REMOTE CTRL] | Displays/hides the ROP app control status. [ON], [OFF] Factory setting: [ON]
[MON OUT MARKER] | [MON OUT1 SW] | Displays/hides markers for the output from the <MON OUT1>. [ON], [OFF] Factory setting: [OFF]
| [MON OUT2 SW] | Displays/hides markers for the output from the <MON OUT2>. [ON], [OFF] Factory setting: [ON]
| [LCD SW] | Displays/hides markers for the control panel. [ON], [OFF] Factory setting: [ON]
| [PB MARKER SW] | Sets whether to superimpose markers to the playback images. The markers to superimpose are the same markers to superimpose to the camera video that is set in [MON OUT MARKER]. [ON], [OFF] Factory setting: [OFF]
| [MARKER & CHAR LVL] | Sets the frame marker and character luminance. Enabled for [FRAME MARK] only when [FRAME COLOR] is set to [WHITE]. [50%]…[100%] (10% step) Factory setting: [70%]
| [CENTER MARKER] | Controls the center mark. [1]: + (large) [2]: Open center (large) [3]: + (medium) [4]: Open center (medium) [5]: + (small) [6]: Open center (small) [7]: + (very small) [OFF]: Does not display. Factory setting: [1]
| [SAFETY MARKER] | Selects the type of frame for the safety zone marker. [1]: Box [2]: Corners [OFF]: Does not display. Factory setting: [OFF]
| [SAFETY AREA] | Sets the size of the safety zone marker. [80%] - [100%] (1% step, fixed aspect ratio) Factory setting: [90%]
| [FRAME MARK] | Enables/disables frame marker. [ON], [OFF] Factory setting: [OFF]
| [FRAME SIG] | Sets frame marker aspect ratio. [1.33:1], [1.44:1], [1.56:1], [1.78:1], [1.85:1], [2.00:1], [2.201:1], [2.35:1], [2.39:1] Factory setting: [2.39:1]
| [FRAME COLOR] | Sets the color of the frame marker. [WHITE], [BLACK], [RED], [GREEN], [BLUE], [YELLOW] Factory setting: [WHITE]
| [FRAME LEVEL] | Sets the level of the outside of the frame marker. [0%] - [100%] (10% step) Factory setting: [100%]
| [USER BOX] | Displays/hides the user box. [ON], [OFF] Factory setting: [OFF]
| [USER BOX WIDTH] | Sets the width of the user box. [1]…[100] Factory setting: [13]
| [USER BOX HEIGHT] | Sets the height of the user box. [1]…[100] Factory setting: [13]
| [USER BOX H POS] | Sets the horizontal position of the center of the user box. [−50]…[50] Factory setting: [0]
| [USER BOX V POS] | Sets the vertical position of the center of the user box. [−50]…[50] Factory setting: [0]
[VF INDICATOR] | [INDICATOR SW] | Sets whether to display items that will be set by [INDICATOR] in the output from the <VF> terminal and <VF SDI> terminal. [ON]: Items are individually displayed/hidden. [OFF]: Hides all. Factory setting: [ON]
| [SYSTEM PIXEL] | Displays/hides system pixels. [ON], [OFF] Factory setting: [ON]
| [SYSTEM FREQ] | Displays/hides system frequency. [ON], [OFF] Factory setting: [ON]
| [REC FORMAT] | Displays/hides recording format display. [ON], [OFF] Factory setting: [ON]
| [REC MODE] | Displays/hides the status for the interval recording or the pre-recording. [ON], [OFF] Factory setting: [ON]
| [VFR] | Displays/hides the variable frame rate status. [ON], [OFF] Factory setting: [ON]
| [FPS] | Displays/hides [FPS]. [ON], [OFF] Factory setting: [ON]
| [SHUTTER] | Displays/hides shutter speed. [ON], [OFF] Factory setting: [ON]
| [EI] | Displays/hides EXPOSURE INDEX. [ON], [OFF] Factory setting: [ON]
| [WHITE] | Displays/hides color temperature. [ON], [OFF] Factory setting: [ON]
| [IRIS] | Displays/hides iris value. [ON], [OFF] Factory setting: [ON]
| [FOCUS] | Displays/hides focus distance. [ON], [OFF] Factory setting: [ON]
| [ZOOM] | Displays/hides zoom value. [ON], [OFF] Factory setting: [ON]
| [FILTER] | Displays/hides the optical filter transmittance. [ON], [OFF] Factory setting: [ON]
| [EXTENDER] | Displays/hides the extender. [ON], [OFF] Factory setting: [ON]
| [Y GET] | Displays/hides brightness of Y GET. [ON], [OFF] Factory setting: [ON]
| [TC] | Displays/hides the time code, user bits, and duration counter displays. [TCG/TCR], [TCG], [OFF] Factory setting: [TCG/TCR]
| [P2 CARD REMAIN] | Displays/hides the display of the remaining recording free space of a P2 card. [ON], [OFF] Factory setting: [ON]
| [BATTERY REMAIN] | Displays/hides the estimated remaining battery charge level. [ON], [OFF] Factory setting: [ON]
| [PROXY] | Displays/hides proxy information. [ON], [OFF] Factory setting: [ON]
| [GPS] | Displays/hides GPS signal reception status. [ON], [OFF] Factory setting: [OFF]
| [REC TALLY] | Displays/hides the method of displaying the recording status. [RED]: The red tally lamp lights up. [GREEN]: The green tally lamp lights up. [CHAR]: The characters [REC] are displayed in the viewfinder. Factory setting: [RED]
| [CLIP NAME] | Displays/hides clip names. [ON], [OFF] Factory setting: [OFF]
| [USER CLIP NAME (TYPE3)] | Switches the display/hide of user clip name when [REC SETTINGS] → [REC METADATA] → [USER CLIP NAME] is set to [TYPE3]. [ON], [OFF] Factory setting: [OFF]
| [INDICATOR OUT SEL] | Selects the output destination of the item to set in the [INDICATOR] page. [VF], [VF SDI], [VF & VF SDI] Factory setting: [VF & VF SDI]
| [REMOTE CTRL] | Displays/hides the ROP app control status. [ON], [OFF] Factory setting: [ON]
[VF MARKER] | [MARKER SW] | Sets whether to display markers in the output from the <VF> terminal and <VF SDI> terminal. [ON], [OFF] Factory setting: [ON]
| [PB MARKER SW] | Sets whether to superimpose markers to the playback images. The markers to superimpose are the same markers to superimpose to the camera video that is set in [MON OUT MARKER]. [ON], [OFF] Factory setting: [OFF]
| [MARKER & CHAR LVL] | Sets the frame marker and character luminance. Enabled for [FRAME MARK]/[SURROUND VIEW] only when [FRAME COLOR]/[-- COLOR SEL] is set to [WHITE]. [50%], [60%], [70%] Factory setting: [50%]
| [CENTER MARKER] | Switches the center marker. [1]: + (large) [2]: Open center (large) [3]: + (medium) [4]: Open center (medium) [5]: + (small) [6]: Open center (small) [7]: + (very small) [OFF]: Does not display. Factory setting: [1]
| [SAFETY MARKER] | Selects the type of frame for the safety zone marker. [1]: Box [2]: Corners [OFF]: Does not display. Factory setting: [OFF]
| [SAFETY AREA] | Sets the size of the safety zone marker. [80] - [100%] (1% step, fixed aspect ratio) Factory setting: [90%]
| [FRAME MARK] | Enables/disables frame marker. [ON], [OFF] Factory setting: [OFF]
| [FRAME SIG] | Sets frame marker aspect ratio. [1.33:1], [1.44:1], [1.56:1], [1.78:1], [1.85:1], [2.00:1], [2.201:1], [2.35:1], [2.39:1] Factory setting: [2.39:1]
| [FRAME COLOR] | Sets the color of the frame marker. [WHITE], [BLACK], [RED], [GREEN], [BLUE], [YELLOW] Factory setting: [WHITE]
| [FRAME LEVEL] | Sets the level of the outside of the frame marker. [0%] - [100%] (10% step) Factory setting: [100%]
| [USER BOX] | Sets whether to display/hide the user box display. [ON], [OFF] Factory setting: [OFF]
| [USER BOX WIDTH] | Sets the width of the user box. [1]…[100] Factory setting: [13]
| [USER BOX HEIGHT] | Sets the height of the user box. [1]…[100] Factory setting: [13]
| [USER BOX H POS] | Sets the horizontal position of the center of the user box. [−50]…[50] Factory setting: [0]
| [USER BOX V POS] | Sets the vertical position of the center of the user box. [−50]…[50] Factory setting: [0]
| [MARKER OUT SEL] | Selects the output destination of the marker display. [VF], [VF SDI], [VF & VF SDI] Factory setting: [VF & VF SDI]
[VF FOCUS ASSIST] | [EXPAND SW] | Displays/hides the enlargement display function. [ON], [OFF] Factory setting: [OFF]
| [- POS] | Adjusts the source signal position in an enlarged display. [0]…[8] Factory setting: [4]
| [- VALUE] | Adjusts the enlargement factor. [x2], [x3], [x4] Factory setting: [x2]
| [- MODE] | Sets the enlargement display function mode. [10SEC], [HOLD], [UNTIL REC] Factory setting: [10SEC]
| [IN COLOR/SQ./MONO SW] | Displays/hides the advanced assist function (peaking and focus square). [ON], [OFF] Factory setting: [OFF]
| [- FOCUS IN COLOR SW] | Displays/hides the peaking function. [ON], [OFF] Factory setting: [OFF]
| [-- PEAKING VALUE] | Sets the peaking function mode. [LOW], [MID], [HIGH] Factory setting: [MID]
| [-- COLOR SEL] | Sets the peaking function color. [RED], [GREEN], [WHITE] Factory setting: [RED]
| [- FOCUS SQUARES SW] | Displays/hides the focus square function. [ON], [OFF] Factory setting: [OFF]
| [- MONO SW] | Enables/disables the monochromatic display function when [IN COLOR/SQ./MONO SW] is set to [ON]. [ON], [OFF] Factory setting: [OFF]
| [FOCUS BAR SW] | Enables/disables the focus bar display function. [ON], [OFF] Factory setting: [ON]
| [IN COLOR/SQ./MONO OUT SEL] | Selects the output destination of the advanced assist function. [VF], [VF SDI], [VF & VF SDI] Factory setting: [VF & VF SDI]
| [FOCUS BAR OUT SEL] | Selects the output destination of the focus bar display. [VF], [VF SDI], [VF & VF SDI] Factory setting: [VF & VF SDI]
[VF EI ASSIST] | [ZEBRA SW] | Sets whether to superimpose the zebra signal on the output from the <VF> terminal and <VF SDI> terminal. [ON], [OFF] Factory setting: [OFF]
| [ZEBRA1 DETECT] | Sets the detection level of zebra pattern 1. [0%] - [109%] Factory setting: [80%]
| [ZEBRA2 DETECT] | Sets the extraction level of zebra pattern 2. [0%] - [109%] Factory setting: [100%]
| [ZEBRA2 MODE] | Enables/disables zebra pattern 2 and selects [SPOT]. [ON], [SPOT], [OFF] Factory setting: [OFF]
| [ZEBRA OUT SEL] | Selects the output destination of the zebra display. [VF], [VF SDI], [VF & VF SDI] Factory setting: [VF & VF SDI]
| [WFM SW] | Displays/hides waveform monitor. [ON]/[OFF] Factory setting: [OFF]
| [- TYPE] | Sets the display format of the waveform monitor. [Y], [YGBR] Factory setting: [Y]
| [- TRANSPARENCE] | Sets the transparency of the waveform monitor display. [0%], [25%], [50%], [75%] Factory setting: [50%]
| [Y GET SW] | Enables/disables the Y GET display function. The user box function will not operate when [Y GET SW] is set to [ON]. [ON], [OFF] Factory setting: [OFF]
| [- UNIT] | Sets the [Y GET] display unit when [MAIN COLOR] is set to [V-Log]. [STOP], [%] Factory setting: [STOP]
| [- AREA SIZE] | Sets the size of area to detect with the Y GET display function. [S], [M], [L] Factory setting: [M]
| [FALSE COLOR SW] | Sets the display of the false color. [ON], [OFF] Factory setting: [OFF]
| [WFM OUT SEL] | Selects the output destination of the waveform monitor display. [VF], [VF SDI], [VF & VF SDI] Factory setting: [VF & VF SDI]
| [FALSE COLOR OUT SEL] | Selects the output destination of the false color display. [VF], [VF SDI], [VF & VF SDI] Factory setting: [VF & VF SDI]

Top of the page