- Top
- Video Recording and Color Grading
- Special recording functions
- Interval recording

# Interval recording

Perform recording at the set time intervals. One frame is recorded at a single recording.

Recording (1 frame)

Recording (1 frame)

Recording (1 frame)

(Time)

Time set in [INTERVAL TIME]

Time set in [INTERVAL TIME]

Set [MENU] → [REC SETTINGS] → [REC FUNCTION] → [REC MODE] to [INTERVAL].

Set the following related items from [MENU] → [REC SETTINGS] → [REC FUNCTION].

- [INTERVAL TIME]: Intermittent time (minimum 2 frames, maximum 1 hour)

- [START DELAY]: Delay time from the time when the <REC> button is pressed until the time when the first recording starts

Press the <REC> button.

Interval recording starts according to the set intermittent time.

- When [INTERVAL TIME] is set to two minutes or longer, the tally lamp flashes every five seconds to indicate that the camera is on standby.

- To stop recording, press the <REC> button.

- To clear settings, set [MENU] → [REC SETTINGS] → [REC FUNCTION] → [REC MODE] to [NORMAL].

- The followings are displayed on the [HOME] screen.

  - During recording: [i REC] lights up in red

  - During pause: [i REC] is inverted in red and white

    When [INTERVAL TIME] is set to less than two seconds, [i REC] lights up in red.

  - During stop: [i REC] in black character

NOTE

- During operation in the interval recording mode, the card access LED of the recording slot flashes in orange. Do not remove this P2 card. If you remove the card, restore the clips. Note that even when the clips are restored, the last three to four seconds of the recording may still be lost (maximum ten seconds in case that the card was removed during recording on multiple P2 cards).

- Pre-recording does not function.

- Audio is not recorded.

- Recorded data (data recorded until the recording was stopped) is included in one file.

Top of the page