- Top
- V-RAW recorder
- Power supply
- Turning on the power

# Turning on the power

#### When turning on the power

Connect the V-RAW recorder.

Connect the battery or the external DC power supply to the V-RAW recorder.

Set the <POWER> switch of the recording module to <ON>.

#### When removing the V-RAW recorder

Set the <POWER> switch of the recording module to <OFF>.

Remove the V-RAW recorder.

NOTE

- When attaching or removing the V-RAW recorder, always turn off the power of the camera main unit before performing. It will cause a system error when the V-RAW recorder is removed with the power turned on.

#### Displaying of the power supply condition

V-RAW recorder | Extension module | The module with lowest power supply level | Battery charge level indicator
--- | --- | --- | ---
No | No | — | —
No | Yes | Recording module |
No | Yes | Camera module |
Yes | No | Recording module |
Yes | No | V-RAW recorder |
Yes | Yes | Recording module |
Yes | Yes | Camera module |
Yes | Yes | V-RAW recorder |

Top of the page