- Top
- Video Recording and Color Grading
- P2 card
- Card access LEDs and P2 card status

# Card access LEDs and P2 card status

Card access LED | P2 card status
--- | ---
Illuminated in green | Recording possible | Reading/writing are both possible.
Illuminated in orange | Recording target | Reading/writing are both possible. The card is currently the recording target (including loop recording).
Flashing in orange | Accessing card | Reading/writing are currently being performed.
Flashing in orange rapidly | The card is being recognized. | The P2 card is being recognized.
Flashing in green slowly | Card full | There is no free space on the P2 card. Reading only is possible.
Write protect | The write-protect switch on the P2 card is at the Protect position. Reading only is possible.
Unrecordable card | Recording is not possible by the currently set recording format since the SD memory card, etc. is inserted. To record the card, change the recording format or use a P2 card.
Off | Card not supported | This card cannot be used on the camera. Replace the card.
Illegal format | The P2 card is not properly formatted. Reformat the card.
No card | The P2 card is not inserted. The card is waiting to be recognized.
Unauthenticated card | An expressP2 memory card or microP2 memory card that cannot be authenticated. Select [MENU] → [SYSTEM SETTINGS] → [CARDS/MEDIA] → [CPS PASSWORD], and enter the password.

Top of the page