- Top
- V-RAW recorder
- Operation with the control panel
- Media

# Media

The Codex media (Capture Drive) is used for the V-RAW recording. Displaying of the various information from the HOME screen, and confirmation of the media status and media format from the INFO screen can be executed from the control panel of the recording module.

## Insertion method of the Capture Drive

Fig. 1

Fig. 2

Fig. 5

Fig. 3

Fig. 4

Open the drive slot cover. (Fig. 1, Fig. 2)

Insert the Capture Drive. (Fig. 3, Fig. 4)

Close the drive slot cover. (Fig. 5)

#### To remove

Fig. 1

Fig. 2

Fig. 3

Open the drive slot cover. (Fig. 1, Fig. 2)

Remove the Capture Drive. (Fig. 3)

NOTE

- Do not remove the Capture Drive while the Capture Drive is being accessed or when the Capture Drive is inserted and being recognized (access LED flashing in blue). Otherwise, it may result in a malfunction.

## Access LED

There is a access LED on the V-RAW recorder and the Capture Drive.

LED status | V-RAW recorder | Capture Drive
--- | --- | ---
Green (illuminated) | Power can be supplied from the V-RAW recorder/camera is powered off | —
Blue (illuminated) | Recording possible | Removing possible
Blue (flashing) | Recording not possible (Capture Drive is being recognized, drive slot cover is opened, etc.) | Capture Drive is being recognized/removing not possible
Red (illuminated) | Recording | —
Red (flashing) | Error has occurred | Capture Drive recognition failed

NOTE

- It may take some time until the access LED for the Capture Drive starts to flash when the Capture Drive is inserted.

- Do not remove the Capture Drive when the access LED is flashing in blue. Otherwise, it may result in a malfunction. The Capture Drive can be removed when the blue flashing turns into blue illumination.

## Recording time of the Capture Drive

The recording time of single Codex Capture Drive 2.0 (2 TB) is as follows.

Resolution | Number of bits | Frame rate | Recording time (minutes)
--- | --- | --- | ---
3840×2160 | 10 bits | 23.98 | 119
3840×2160 | 10 bits | 25 | 114
3840×2160 | 10 bits | 29.97/30 | 95
3840×2160 | 10 bits | 48 | 59
3840×2160 | 10 bits | 50 | 57
3840×2160 | 10 bits | 59.94/60 | 47
3840×2160 | 10 bits | 96 | 29
3840×2160 | 10 bits | 120 | 23
3840×2160 | 12 bits | 23.98 | 106
3840×2160 | 12 bits | 25 | 101
3840×2160 | 12 bits | 29.97/30 | 84
4096×2160 | 10 bits | 23.98/24 | 112
4096×2160 | 10 bits | 25 | 107
4096×2160 | 10 bits | 29.97/30 | 89
4096×2160 | 10 bits | 48 | 56
4096×2160 | 10 bits | 50 | 53
4096×2160 | 10 bits | 59.94/60 | 44
4096×2160 | 10 bits | 96 | 28
4096×2160 | 10 bits | 120 | 22
4096×2160 | 12 bits | 23.98/24 | 100
4096×2160 | 12 bits | 25 | 96
4096×2160 | 12 bits | 29.97/30 | 80

## Formatting of the Capture Drive

Perform from the INFO screen in the control panel.

#### To operate from MENU

Select [V-RAW] in [MENU] → [SYSTEM SETTINGS] → [CARDS/MEDIA] → [FORMAT MEDIA].

Select [YES] using the jog dial button.

NOTE

- Data deleted as a result of formatting cannot be restored. Always check the data before formatting.

Top of the page