- Top
- Other Useful Functions
- Setting the time data
- How to input user bits

# How to input user bits

By setting user bits, information such as memos (date, time) up to eight digits long (hexadecimal) can be recorded.

Press the <TC> button to display the TC screen.

From the user bits display, select [User] in [UB MODE].

Select [SET].

The [TC SET] screen is displayed.

Set the user bits using the jog dial button.

Press the jog dial button to confirm the user bits setting value.

NOTE

- If you exit the user bits setting screen without pressing the jog dial button, the set values will be disabled.

## Retention of user bits in memory

User bit settings are automatically recorded and are retained even if the power is turned off.

## Frame rate information

The relationship between frame rates, image pull-down, and time codes/user bits is as follows.

Media management information

Fixed values

Verification information on the right-hand six digits

Updated frame flags and valid frame flags

REC mark

Sequence No.

24P: 0-4

Other than above: F-fixed

Camera image mode

Example)

(During shooting)

(VFR 30PN or over 60P)

(VFR over 60P)

(VFR 24PN during shooting)

(VFR 25PN or over 50P)

Top of the page