- Top
- Specification
- Specifications
- Specifications

# Specifications

## General

Power DC 12 V (11.0 V - 17.0 V) Power consumption 99 W (with all optional accessories connected and maximum power supplied from each output terminal)

indicates safety information.

Ambient operating temperature | 0 °C - 40 °C (32 °F - 104 °F)
Ambient operating humidity | 10% - 85% (relative humidity)
Storage temperature | −20 °C - 60 °C (−4 °F - 140 °F)
Weight | Approx. 5.0 kg (11.02 lbs.) (excluding accessories)
Dimensions (W×H×D) | Body only 179.0 mm×230.5 mm×347.0 mm (7-1/16 inches×9-3/32 inches×13-11/32 inches) (excluding protrusions and accessories)

- Ensure that the total current from the <DC OUT> terminal, <VF> terminal, and <LENS> terminal of the camera module, and the <DC OUT/RS> terminal and <USB HOST> terminal of the recording module does not exceed 30 W.

## Camera unit

Pickup device | Super 35 mm, MOS, 8.9 megapixels
Number of pixels | Total number of pixels Approx. 10.3 million pixels Number of effective pixels Approx. 8.9 million pixels
Lens mount | 35 mm, PL mount
Optical filter | ND filter <1>: <CLEAR>, <2>: <0.6ND>, <3>: <1.2ND>, <4>: <1.8ND>
Gain setting | [ISO] mode ISO200 - ISO12800 [dB] mode 0 dB - 24 dB (3 dBstep)
Shutter speed | [deg] mode 1.0 deg - 358 deg (0.5 deg step) [sec] mode 1/24 seconds - 1/250 seconds (for 24p)

## Memory card recorder

Recording media | expressP2 memory card, P2 memory card, microP2 memory card
Number of recording pixels | 4096×2160, 3840×2160, 2048×1080, 1920×1080
Recording frame rate (max) | 4K 100p/120p HD 100p/120p
System frequency | 59.94p, 50p, 29.97p, 25p, 24p, 23.98p, 59.94i, 50i
Recording format (main recorder) | AVC-Intra 4K 444/AVC-Intra 4K 422/AVC-Intra 4K-LT/AVC-Intra 2K 444/AVC-Intra 2K 422/AVC-Intra 444/AVC-Intra 200/AVC-Intra 422/AVC-Intra 100/ProRes 4444 XQ/ProRes 4444/ProRes 422 HQ/ProRes 422/ProRes 422 LT
Recording format (sub recorder) | AVC-Intra 2K 422/AVC-Intra 422/AVC-Intra 100/AVC-LongG 50/AVC-LongG 25
Recording video signal | 4096×2160/59.94p, 50p, 29.97p, 25p, 24p, 23.98p 3840×2160/59.94p, 50p, 29.97p, 25p, 23.98p 2048×1080/59.94p, 50p, 29.97p, 25p, 24p, 23.98p 1920×1080/59.94p, 50p, 29.97p, 25p, 23.98p, 59.94i, 50i
Recording and playback time ([MAIN CODEC]) | When using a 256 GB expressP2 memory card AVC-Intra 4K 444, 24p Approx. 45 min AVC-Intra 4K 422, [VFR]: [ON], 50 fps/60 fps Approx. 36 min AVC-Intra 4K 422, [VFR]: [OFF], 24p Approx. 90 min AVC-Intra 4K-LT, [VFR]: [ON], 100 fps/120 fps Approx. 32 min AVC-Intra 100, [VFR]: [ON], 100 fps/120 fps Approx. 64 min ProRes 422 HQ, [VFR]: [ON], 60 fps Approx. 60 min
Figures are for continuous recording as one clip. Depending on the number of clips, the overall recording time may be shorter than the above.
Recording and playback time ([SUB CODEC]) | When using a 64 GB microP2 memory card AVC-Intra 2K 422, 25.00p/29.97p Approx. 64 min AVC-Intra 100, 25.00p/29.97p Approx. 64 min AVC-LongG 50, 25.00p/29.97p Approx. 128 min AVC-LongG 25, 25.00p/29.97p Approx. 256 min
Figures are for continuous recording as one clip. Depending on the number of clips, the overall recording time may be shorter than the above.

## Digital video

Number of quantizing bits | 12 bit (AVC-Intra 4K 444/AVC-Intra 2K 444/AVC-Intra 444), 10 bit (others)
Video compression format | AVC-Intra 4K 444/AVC-Intra 4K 422/AVC-Intra 4K-LT/AVC-Intra 2K 444/AVC-Intra 2K 422/AVC-Intra 444/AVC-Intra 200/AVC-Intra 422/AVC-Intra 100 MPEG-4 AVC/H.264 Intra Profile AVC-LongG 50/AVC-LongG 25 MPEG-4 AVC/H.264 ProRes 4444 XQ/ProRes 4444/ProRes 422 HQ/ProRes 422/ProRes 422 LT Apple ProRes

## Digital audio

Recording audio signal | 48 kHz/24 bits, 4CH
Headroom | 18 dB/20 dB switchable menu

## Proxy

File format | MOV
Video compression format | H.264/AVC High Profile
Audio compression format | LPCM
Approximate recording time (1 GB) | Approx. 25 min
Reference value for continuous recording. The recording time may differ depending on the scene or the number of clips.

## Video input/output

<SDI OUT1>/<SDI OUT2>/<SDI OUT3>/<SDI OUT4> terminal | HD (1.5G)/3G-SDI: 0.8 V [p-p], 75 Ω (1 set, 4 pieces)
<MON OUT1> terminal | HD (1.5G)/3G-SDI: 0.8 V [p-p], 75 Ω
<MON OUT2> terminal | HD (1.5G)/3G-SDI: 0.8 V [p-p], 75 Ω
<VF SDI> terminal | HD (1.5G)/3G-SDI: 0.8 V [p-p], 75 Ω

## Audio input/output

<AUDIO IN 1>/<AUDIO IN 2> terminal | XLR×2, 3-pin <LINE>/<MIC>/<MIC+48V>/<AES> switchable type
<MIC IN> terminal | XLR×1, 5-pin
<PHONES> terminal | Stereo mini jack
Speaker | 20 mm diameter, round ×1

## Viewfinder

Display panel | OLED (organic EL) 0.7 type, 2760000 dots
Video input method | 1080/59.94p, 1080/50p, 1080/60p

## Other input/output

<GENLOCK IN> terminal | HD (1.5G)/3G-SDI: 0.8 V [p-p], 75 Ω
<TC IN/OUT> terminal | BNC×1 Input/output switching Input: 0.5 V - 8 V [p-p], 10 kΩ Output: 2.0 V±0.5 V [p-p], low impedance
<DC IN> terminal | XLR×1, 4-pin, DC 12 V (DC 11.0 V - 17.0 V)
<DC OUT/RS> terminal | 4-pin, DC 12 V (DC 11.0 V - 17.0 V), maximum output current 1.0 A
<DC OUT> terminal | 2-pin, DC 12 V (DC 11.0 V - 17.0 V), maximum output current 1.0 A
<LENS> terminal | 12-pin, 4-pin×2
<VF> terminal | 14-pin
<LAN> terminal | 100BASE-TX/10BASE-T
<USB2.0> terminal (device) | Type B connector, 4-pin
<USB2.0> terminal (host) | Type A connector, 4-pin
<EXT> terminal | 50-pin, exclusive for external recording (to be supported)
Control panel (LCD) | 3.5-type QHD color monitor (approx. 1.56 million dots)

Top of the page