- Top
- Other Useful Functions
- Assigning functions to the USER buttons
- Selectable functions

# Selectable functions

Item | Description
--- | ---
[INHIBIT] | Disables assignment of functions.
[SIX USER BUTTONS] | Sets against the USER <1> to <4> buttons, when the control panel operation button is used as the USER button.
[AWB] | Assigns the automatic white balance function.
[ABB] | Assigns the automatic black balance function.
[Y GET] | Assigns the function for displaying the luminance level of the image at the position indicated by the square marker displayed near the center.
[EXPAND] | Assigns the enlargement function.
[IN COLOR/SQ./MONO] | Switches ON/OFF of the focus in color function, the focus square function, and the monochrome display function.
[WFM] | Enables/disables the viewfinder wave form display.
[BARS] | Assigns the color bars display function.
[FRAME LINE] | Displays/hides the frame line display function.
[FALSE COLOR] | Enables/disables the false color mode.
[VF COLOR] | Switches output images from the viewfinder and the <VF SDI> terminal.
[MON1 COLOR] | Switches output images from the <MON OUT1> terminal.
[MON2 COLOR] | Switches output images from the <MON OUT2> terminal.
[VF DESQUEEZE] | Switches ON/OFF of the de-squeeze function against the viewfinder and the output from the <VF SDI> terminal.
[VF IMAGE INVERT] | Switches ON/OFF of the invert display function against the viewfinder and the output from the <VF SDI> terminal.
[SMOOTH MODE] | Assigns the smooth mode function.
[TEXT MEMO] | Assigns the text memo function.
[SHOT MARK] | Assigns the shot mark function.
[MAIN SLOT SEL] | Assigns the function for switching the card for recording when two or more cards are inserted in the main slot.
[SUB SLOT SEL] | Assigns the function for switching the card for recording when two or more cards are inserted in the sub slot.
[REC SW] | Assigns the function of the <REC> button.
[AUDIO MON VOL] | Calls out the screen to adjust the monitor output of audio to the control panel.
[AUDIO IN VOL] | Calls out the screen to adjust the input of audio to the control panel.
[VFR SW] | Enables/disables the variable frame rate function.
[CHECK LAST CLIP START] | Plays back the first 5 seconds of the newest clip of the clips recorded in the main recorder after the power was turned on. Enabled only in the HOME screen or the VIEW screen.
[CHECK LAST CLIP END] | Plays back the last 5 seconds of the newest clip of the clips recorded in the main recorder after the power was turned on. Enabled only in the HOME screen or the VIEW screen.

NOTE

- Only the following functions can be assigned to [USER5] to [USER10].

  [INHIBIT], [EXPAND], [IN COLOR/SQ./MONO], [FRAME LINE], [VF COLOR], [MON1 COLOR], [MON2 COLOR], [SMOOTH MODE], [VFR SW]

Top of the page