- Top
- Maintenance
- Warning system
- Cases indicated by error codes

# Cases indicated by error codes

Error code | Display | Description | Behavior and cause
--- | --- | --- | ---
[E-30] | [TURN POWER OFF] | An error occurred in the camera built-in memory because the P2 card being accessed was ejected. Warning lamp flashes four times per second. | Cannot operate. Follow the message to turn off the power once and turn on the power again. Ensure that there is no error in the clips on the ejected card, and restore the clips as necessary.
[E-31] | [TURN POWER OFF] | System mode error occurred. Warning lamp flashes four times per second. | Cannot operate. Follow the message to turn off the power once, turn on the power again, and check that there is no error display.
[E-33] | [SYSTEM ERROR] | Camera unit error occurred. Warning lamp flashes four times per second. | The operation stops. Contact your dealer.
[E-35] | [SYSTEM ERROR] | Codec control error occurred. Warning lamp flashes four times per second. | The operation stops. Contact your dealer.
[E-36] | [SYSTEM ERROR] | P2 system error occurred. Warning lamp flashes four times per second. | The operation stops. When it occurs right after the power is turned on after connecting the V-RAW recorder, and the LED of the V-RAW recorder stays illuminated in green Turn off the power of the V-RAW recorder once, and then turn on the power again after removing the Capture Drive. Contact your dealer.
[E-37] | [SYSTEM ERROR] | P2CS microcomputer error occurred. Warning lamp flashes four times per second. | The operation stops. Contact your dealer.
[E-39] | [SYSTEM ERROR] | Video initialization error occurred. Warning lamp flashes four times per second. | The operation stops. Contact your dealer.
[E-64] | [SYSTEM ERROR] (or no display) | Reference signal error occurred. Warning lamp flashes four times per second. | The operation stops. Contact your dealer.
[E-65] | [No Camera Module Detected] | The camera module cannot be recognized. Warning lamp flashes four times per second. | The operation will stop. Contact your dealer.
[E-67] | [Check Camera Module Connection] | There is a connection error between the camera module and the recording module. Warning lamp flashes four times per second. | The operation will stop. Confirm if the cable connectors are connected correctly when the extension module is used. Contact your dealer.

Top of the page