- Top
- Extension module
- Power supply
- Battery attachment and setting

# Battery attachment and setting

## Using Anton/Bauer batteries

Release lever

Anton/Bauer batteries

Mount the Anton/Bauer battery.

Insert the battery terminal and slide in the direction of the arrow.

Set the battery features.

Select [CAM BATT FULL]/[CAM BATT NEAR END]/[CAM BATT END] in [MENU] → [SYSTEM SETTINGS] → [BATTERY] to set the voltage at which the battery level and warning will be displayed.

NOTE

- To remove the battery, keep the release lever of the battery holder completely down, slide the battery in the opposite direction when you mounted it.

## Using V-mount type batteries

Mount the V-mount type battery plate. As shown in the illustration, insert and slide in the direction of the arrow.

Release lever

Mount the V-mount type battery plate.

Slide in the direction of the arrow.

Set the battery features.

- Select [CAM BATT FULL]/[CAM BATT NEAR END]/[CAM BATT END] in [MENU] → [SYSTEM SETTINGS] → [BATTERY] to set the voltage at which the battery level and warning will be displayed.

NOTE

- Contact your dealer for information about the V-mount type battery plate.

- When removing the plate, remove by sliding the release lever.

Top of the page